Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2152	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Barry, Earl	Locality:
	Date Desc.:	02/08/93	Elevation:	No Data
	Map Ref.:	Sheet No. : 8155   GPS	Rainfall:	No Data
	Northing/Long.:	7677218 AMG zone: 55	Runoff:	Slow
	Easting/Lat.:	440388  Datum: AGD66	Drainage:	Moderately well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Plain
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	1 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Eutrophic Brown Dermosol Thick Non-gravelly Silty 	Principal Profile Form:	Db1.13
	Clayey Deep
	ASC Confidence:	Great Soil Group:	Brown earth
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.51-1m, Mid-dense. *Species includes - Bothriochloa species
	Mid Strata - Tree, 3.01-6m, Very sparse. *Species includes - Eucalyptus brownii, Atalaya hemiglauca
	Tall Strata - Tree, 12.01-20m, Sparse. *Species includes - Eucalyptus brownii, Eucalyptus erythrophloia
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A11	0 - 0.38 m	Very dark greyish brown (10YR3/2-Moist); ; Silty clay loam; Massive grade of structure; Earthy 
	fabric; Dry; Strong consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.15); 
	Clear change to - 
	B21	0.38 - 0.7 m	Dark brown (10YR3/3-Moist); ; Medium clay; Moderate grade of structure, 10-20 mm, Polyhedral; 
	Smooth-ped fabric; Dry; Strong consistence; Very few (0 - 2 %), Ferromanganiferous, Fine (0 - 2 
	mm), Nodules; , Calcareous, , ; , Gypseous, , ; Field pH 6.5 (Raupach, 0.5); Gradual change to - 
	B22	0.7 - 1 m	Brown (10YR4/3-Moist); ; Light medium clay; Dry; 20-50%, coarse gravelly, 20-60mm, 
	subangular, Limestone, coarse fragments; Few (2 - 10 %), Ferromanganiferous, Medium (2 -6 
	mm), Nodules; , Calcareous, , ; , Gypseous, , ; Field pH 8.5 (Raupach, 0.8); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2152	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2152	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile