Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2160	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Barry, Earl	Locality:
	Date Desc.:	03/08/93	Elevation:	No Data
	Map Ref.:	Sheet No. : 8254   GPS	Rainfall:	No Data
	Northing/Long.:	7617083 AMG zone: 55	Runoff:	Rapid
	Easting/Lat.:	449978  Datum: AGD66	Drainage:	Moderately well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, Sandstone 
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  1-	Pattern Type:	Plain
	3%
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Very gently sloped
	Slope:	3 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Eutrophic Red Dermosol     	Principal Profile Form:	Uf6.31
	ASC Confidence:	Great Soil Group:	No suitable 
	No analytical data are available but confidence is fair.
	Site Disturbance:	Extensive clearing, for example poisoning, ringbarking
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Very sparse. *Species includes - None recorded
	Mid Strata - , , . *Species includes - None recorded
	Tall Strata - Tree, 6.01-12m, Very sparse. *Species includes - Eucalyptus papuana, Eucalyptus brownii
	Surface Coarse Fragments:	10-20%, cobbly, 60-200mm, subangular platy, Sandstone
	Profile Morphology
	A11	0 - 0.06 m	Dark brown (10YR3/3-Moist); ; Light clay; Massive grade of structure; Earthy fabric; Dry; Very 
	firm consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.03); 
	B21	0.06 - 0.5 m	Dark reddish brown (5YR3/4-Moist); ; Medium heavy clay; Moderate grade of structure, 20-50 
	mm, Angular blocky; Smooth-ped fabric; Dry; Very strong consistence; 2-10%, medium gravelly,
	 6-20mm, subangular, Sandstone, coarse fragments; , Calcareous, , ; , Gypseous, , ; Field pH 6 
	(Raupach, 0.4); Field pH 6.5 (Raupach, 0.5); 
	C	0.5 - 0.6 m	; Dry; , Calcareous, , ; , Gypseous, , ; 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2160	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2160	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile