Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2165	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Barry, Earl	Locality:
	Date Desc.:	04/08/93	Elevation:	No Data
	Map Ref.:	Sheet No. : 8155   GPS	Rainfall:	No Data
	Northing/Long.:	7624720 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	437407  Datum: AGD66	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, Calcrete 
	Land Form
	Rel/Slope Class: 	Undulating plains <9m 3-10%	Pattern Type:	Plain
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Gently inclined
	Slope:	4 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Soft
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Calcic Red Dermosol     	Principal Profile Form:	Gn4.13
	ASC Confidence:	Great Soil Group:	No suitable 
	No analytical data are available but confidence is fair.
	Site Disturbance:	Limited clearing, for example selective logging
	Vegetation:	Low Strata - Tussock grass, 0.51-1m, Sparse. *Species includes - Eriachne species, Chrysopogon fallax, Dichanthium 
	species	Mid Strata - Tree, 3.01-6m, Sparse. *Species includes - Bursaria incana, Lysiphillum carronii
	Tall Strata - Tree, 12.01-20m, Sparse. *Species includes - Bloodwood, Eucalyptus papuana, Eucalyptus melanophloia
	Surface Coarse Fragments:	2-10%, coarse gravelly, 20-60mm, subangular, Calcrete
	Profile Morphology
	A11	0 - 0.08 m	Dark reddish brown (5YR3/2-Moist); ; Sandy clay loam; Massive grade of structure; Earthy 
	fabric; Firm consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6.5 (Raupach, 0.05); Clear 
	B1	0.08 - 0.25 m	Dark reddish brown (2.5YR2/3-Moist); ; Sandy light clay; Massive grade of structure; Earthy 
	fabric; Firm consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6.5 (Raupach, 0.2); Gradual 
	change to - 
	B21	0.25 - 0.6 m	Dark red (10R3/6-Moist); ; Sandy light medium clay; Moderate grade of structure, 20-50 mm, 
	Subangular blocky; Rough-ped fabric; Strong consistence; , Calcareous, , ; , Gypseous, , ; Field
	 pH 6 (Raupach, 0.5); 
	B22	0.6 - 1 m	Dark red (10R3/6-Moist); ; Sandy light medium clay; Very few (0 - 2 %), Calcareous, Medium (2 
	-6 mm), Soft segregations; , Gypseous, , ; Field pH 6.5 (Raupach, 0.9); 
	C	1 - 1.5 m	; , Calcareous, , ; , Gypseous, , ; Field pH 8.5 (Raupach, 1.5); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2165	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2165	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile