Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2166	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Barry, Earl	Locality:
	Date Desc.:	04/08/93	Elevation:	No Data
	Map Ref.:	Sheet No. : 8155   GPS	Rainfall:	No Data
	Northing/Long.:	7638230 AMG zone: 55	Runoff:	Slow
	Easting/Lat.:	408126  Datum: AGD66	Drainage:	Well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Plain
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	1 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Soft
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Eutrophic Yellow Kandosol     	Principal Profile Form:	Gn1.35
	ASC Confidence:	Great Soil Group:	N/A
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.51-1m, Sparse. *Species includes - Aristida species
	Mid Strata - Tree, 3.01-6m, Sparse. *Species includes - Acacia species, Melaleuca nervosa, Eucalyptus setosa
	Tall Strata - Tree, 12.01-20m, Very sparse. *Species includes - Eucalyptus papuana
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A11	0 - 0.12 m	Black (10YR2/1-Moist); ; Loamy sand; Massive grade of structure; Earthy fabric; Dry; Very 
	weak consistence; , Calcareous, , ; , Gypseous, , ; Field pH 7 (Raupach, 0.05); Clear change to 
	A12	0.12 - 0.3 m	Dark yellowish brown (10YR4/4-Moist); ; Loamy sand; Single grain grade of structure; Dry; 
	Very weak consistence; , Calcareous, , ; , Gypseous, , ; Field pH 7 (Raupach, 0.2); Gradual 
	change to - 
	A2e	0.3 - 0.6 m	Yellowish brown (10YR5/4-Moist); ; Clayey sand; Single grain grade of structure; Dry; Very 
	weak consistence; , Calcareous, , ; , Gypseous, , ; Field pH 7 (Raupach, 0.4); Gradual change 
	B1	0.6 - 0.9 m	Red (2.5YR5/6-Moist); ; Sandy loam; Single grain grade of structure; Dry; Very weak 
	consistence; , Calcareous, , ; , Gypseous, , ; Field pH 7 (Raupach, 0.8); Gradual change to - 
	B21	0.9 - 1 m	Brownish yellow (10YR6/6-Moist); ; Sandy clay loam (Heavy); Single grain grade of structure; 
	Dry; Very weak consistence; , Calcareous, , ; , Gypseous, , ; Field pH 7 (Raupach, 1); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2166	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2166	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile