Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2180	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Barry, Earl	Locality:
	Date Desc.:	06/08/93	Elevation:	No Data
	Map Ref.:	Sheet No. : 8155   GPS	Rainfall:	No Data
	Northing/Long.:	7651445 AMG zone: 55	Runoff:	Rapid
	Easting/Lat.:	448439  Datum: AGD66	Drainage:	Moderately well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  1-	Pattern Type:	Plain
	3%
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Very gently sloped
	Slope:	2 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Eutrophic Brown Kandosol     	Principal Profile Form:	Gn4.82
	ASC Confidence:	Great Soil Group:	No suitable 
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, <0.25m, Isolated plants. *Species includes - None recorded
	Mid Strata - , , . *Species includes - None recorded
	Tall Strata - Tree, 3.01-6m, Very sparse. *Species includes - Eucalyptus melanophloia
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A11	0 - 0.1 m	Very dark greyish brown (10YR3/2-Moist); ; Clay loam, fine sandy; Massive grade of structure; 
	Earthy fabric; Very firm consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6.5 (Raupach, 
	0.05); Clear change to - 
	B1	0.1 - 0.32 m	Dark brown (10YR3/3-Moist); ; Fine sandy light clay; Massive grade of structure; Earthy fabric; 
	Strong consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6.5 (Raupach, 0.25); Gradual 
	change to - 
	B21	0.32 - 0.65 m	Yellowish brown (10YR5/6-Moist); ; Light clay; Massive grade of structure; Earthy fabric; 
	Strong consistence; , Calcareous, , ; , Gypseous, , ; Field pH 7 (Raupach, 0.5); Gradual change 
	B22	0.65 - 0.9 m	Red (2.5YR5/6-Moist); ; Light medium clay; Weak grade of structure, 10-20 mm, Subangular 
	blocky; Rough-ped fabric; Very strong consistence; , Calcareous, , ; , Gypseous, , ; Field pH 7 
	(Raupach, 0.8); 
	B23	0.9 - 1.2 m	Strong brown (7.5YR4/6-Moist); ; Light medium clay; , Calcareous, , ; , Gypseous, , ; Field pH 7 
	(Raupach, 1.1); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2180	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2180	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile