Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2189	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Barry, Earl	Locality:
	Date Desc.:	24/08/93	Elevation:	No Data
	Map Ref.:	Sheet No. : 7859   GPS	Rainfall:	No Data
	Northing/Long.:	7883147 AMG zone: 55	Runoff:	Rapid
	Easting/Lat.:	286889  Datum: AGD66	Drainage:	Imperfectly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, No Data
	Land Form
	Rel/Slope Class: 	Undulating rises 9-30m 3-10%	Pattern Type:	Rises
	Morph. Type:	Lower-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	Gently inclined
	Slope:	4 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Eutrophic Brown Dermosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	N/A
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Very sparse. *Species includes - Bothriochloa species, Aristida species
	Mid Strata - Tree, 1.01-3m, Sparse. *Species includes - Eucalyptus brownii
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - Eucalyptus brownii
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.08 m	Brown (10YR4/3-Moist); ; Fine sandy clay loam; Massive grade of structure; Earthy fabric; Dry; 
	Very firm consistence; 0-2%, fine gravelly, 2-6mm, subangular, Quartz, coarse fragments; , 
	Calcareous, , ; , Gypseous, , ; Field pH 5.5 (Raupach, 0.04); Abrupt change to - 
	A2e	0.08 - 0.18 m	Brown (10YR5/3-Moist); ; Clay loam, fine sandy; Massive grade of structure; Earthy fabric; Dry;
	 Very firm consistence; 0-2%, fine gravelly, 2-6mm, subangular, Quartz, coarse fragments; , 
	Calcareous, , ; , Gypseous, , ; Field pH 5.5 (Raupach, 0.1); Abrupt change to - 
	B1	0.18 - 0.28 m	Dark yellowish brown (10YR4/4-Moist); ; Light medium clay; Massive grade of structure; Earthy 
	fabric; Dry; Strong consistence; 0-2%, fine gravelly, 2-6mm, subangular, Quartz, coarse 
	fragments; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.25); Clear change to - 
	B21	0.28 - 0.45 m	Reddish brown (2.5YR4/4-Moist); Mottles, 10YR44, 0-2% , 5-15mm, Faint; Mottles, 0-2% ; 
	Medium clay; Weak grade of structure, 5-10 mm, Polyhedral; Smooth-ped fabric; Dry; Very firm 
	consistence; 0-2%, fine gravelly, 2-6mm, subangular, Quartz, coarse fragments; Very few (0 - 
	2 %), Manganiferous, , Nodules; , Calcareous, , ; , Gypseous, , ; Field pH 7 (Raupach, 0.45); 
	Gradual change to - 
	B23	0.45 - 1 m	; Moderate grade of structure, 10-20 mm, Subangular blocky; Smooth-ped fabric; Dry; , 
	Calcareous, , ; , Gypseous, , ; Field pH 9 (Raupach, 0.8); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2189	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2189	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile