Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2205	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Barry, Earl	Locality:
	Date Desc.:	26/08/93	Elevation:	No Data
	Map Ref.:	Sheet No. : 7859   GPS	Rainfall:	No Data
	Northing/Long.:	7857578 AMG zone: 55	Runoff:	Rapid
	Easting/Lat.:	265957  Datum: AGD66	Drainage:	Rapidly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Undulating rises 9-30m 3-10%	Pattern Type:	Rises
	Morph. Type:	Upper-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	Gently inclined
	Slope:	6 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Calcic Red Dermosol Thin Moderately gravelly Clay-	Principal Profile Form:	Gn3
	loamy Clayey Moderately deep
	ASC Confidence:	Great Soil Group:	N/A
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Very sparse. *Species includes - Chrysopogon fallax
	Mid Strata - , , . *Species includes - None recorded
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - Eucalyptus crebra, Eucalyptus erythrophloia, Eucalyptus 
	Surface Coarse Fragments:	20-50%, coarse gravelly, 20-60mm, subangular, Graywacke
	Profile Morphology
	A11	0 - 0.05 m	Dark olive (5Y3/3-Moist); ; Clay loam, sandy; Massive grade of structure; Earthy fabric; Dry; 
	Very firm consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.02); Abrupt 
	B1	0.05 - 0.15 m	Dark reddish brown (2.5YR3/4-Moist); ; Light clay; Moderate grade of structure, 10-20 mm, 
	Subangular blocky; Moderate grade of structure, 2-5 mm, Polyhedral; Rough-ped fabric; 
	Moderately moist; Very strong consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6 
	(Raupach, 0.1); Clear change to - 
	B21	0.15 - 0.4 m	Reddish brown (2.5YR4/4-Moist); ; Light medium clay; Moderate grade of structure, 10-20 mm, 
	Angular blocky; Smooth-ped fabric; Moderately moist; Very firm consistence; , Calcareous, , ; , 
	Gypseous, , ; Field pH 6.5 (Raupach, 0.3); Clear change to - 
	B22	0.4 - 0.8 m	Weak red (10R4/4-Moist); ; Light medium clay; Moderate grade of structure, 10-20 mm, Angular 
	blocky; Smooth-ped fabric; Dry; Very firm consistence; Very few (0 - 2 %), Calcareous, 
	Coarse (6 - 20 mm), Nodules; , Gypseous, , ; Field pH 8.5 (Raupach, 0.7); Gradual change to - 
	B23	0.8 - 1.1 m	Weak red (10R4/4-Moist); ; Light clay; Smooth-ped fabric; Dry; Very firm consistence; , 
	Calcareous, , ; , Gypseous, , ; Field pH 9 (Raupach, 1.1); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2205	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2205	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile