Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2206	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Barry, Earl	Locality:
	Date Desc.:	27/08/93	Elevation:	No Data
	Map Ref.:	Sheet No. : 7859   GPS	Rainfall:	No Data
	Northing/Long.:	7851016 AMG zone: 55	Runoff:	Rapid
	Easting/Lat.:	269699  Datum: AGD66	Drainage:	Well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, Shale 
	Land Form
	Rel/Slope Class: 	Undulating rises 9-30m 3-10%	Pattern Type:	Rises
	Morph. Type:	Upper-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	Gently inclined
	Slope:	5 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Eutrophic Red Dermosol Medium Non-gravelly Clay-	Principal Profile Form:	Gn3.13
	loamy Clayey Moderately deep
	ASC Confidence:	Great Soil Group:	N/A
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.51-1m, Sparse. *Species includes - Bothriochloa decipiens, Heteropogon contortus
	Mid Strata - Tree, 6.01-12m, Sparse. *Species includes - Eucalyptus crebra, Eucalyptus papuana
	Tall Strata - Tree, 12.01-20m, Sparse. *Species includes - Eucalyptus crebra
	Surface Coarse Fragments:	0-2%, coarse gravelly, 20-60mm, subangular, Quartz
	Profile Morphology
	A11	0 - 0.1 m	Dark reddish brown (5YR3/4-Moist); ; Clay loam; Massive grade of structure; Earthy fabric; Dry;
	 Strong consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6.5 (Raupach, 0.05); Clear 
	change to - 
	B1	0.1 - 0.22 m	Reddish brown (5YR4/4-Moist); ; Light clay; Weak grade of structure, 2-5 mm, Polyhedral; 
	Smooth-ped fabric; Dry; Very strong consistence; 0-2%, medium gravelly, 6-20mm, subangular 
	platy, Shale, coarse fragments; , Calcareous, , ; , Gypseous, , ; Field pH 6.5 (Raupach, 0.2); 
	Clear change to - 
	B21	0.22 - 0.4 m	Yellowish red (5YR4/6-Moist); ; Medium clay; Moderate grade of structure, 10-20 mm, 
	Polyhedral; Moderate grade of structure, 2-5 mm, Polyhedral; Smooth-ped fabric; Moderately 
	moist; Very strong consistence; 0-2%, medium gravelly, 6-20mm, subangular platy, Shale, 
	coarse fragments; Very few (0 - 2 %), Manganiferous, Fine (0 - 2 mm), Laminae; , Calcareous, 
	, ; , Gypseous, , ; Field pH 7 (Raupach, 0.38); Diffuse change to - 
	BC	0.4 - 0.78 m	Yellowish red (5YR5/6-Moist); ; Light medium clay; Moderate grade of structure, 10-20 mm, 
	Platy; Smooth-ped fabric; Dry; Very firm consistence; 2-10%, coarse gravelly, 20-60mm, 
	subangular platy, Shale, coarse fragments; Few (2 - 10 %), Manganiferous, Fine (0 - 2 mm), 
	Laminae; , Calcareous, , ; , Gypseous, , ; Field pH 7 (Raupach, 0.7); Diffuse change to - 
	C	0.78 - 0.9 m	; Light clay; Dry; , Calcareous, , ; , Gypseous, , ; Field pH 8 (Raupach, 0.9); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2206	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2206	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile