Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2213	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Barry, Earl	Locality:
	Date Desc.:	21/10/93	Elevation:	No Data
	Map Ref.:	Sheet No. : 7959   GPS	Rainfall:	No Data
	Northing/Long.:	7887633 AMG zone: 55	Runoff:	Rapid
	Easting/Lat.:	299876  Datum: AGD66	Drainage:	Well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Rolling rises 9-30m 10-32%	Pattern Type:	Rises
	Morph. Type:	Mid-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	Moderately inclined
	Slope:	11 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Mottled Eutrophic Red Dermosol Medium Very gravelly Clay-	Principal Profile Form:	Gn3.11
	loamy Clayey Moderately deep
	ASC Confidence:	Great Soil Group:	No suitable 
	Analytical data are incomplete but reasonable confidence.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Very sparse. *Species includes - Themeda triandra
	Mid Strata - , , . *Species includes - None recorded
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - Eucalyptus melanophloia, Eucalyptus crebra
	Surface Coarse Fragments:	50-90%, coarse gravelly, 20-60mm, angular, Jasper
	Profile Morphology
	A1	0 - 0.1 m	Brown (7.5YR4/3-Moist); ; Clay loam; Massive grade of structure; Earthy fabric; Dry; Weak 
	consistence; 20-50%, coarse gravelly, 20-60mm, angular, Jasper, coarse fragments; , 
	Calcareous, , ; , Gypseous, , ; Field pH 6.5 (Raupach, 0.05); Clear change to - 
	B1	0.1 - 0.25 m	Reddish brown (5YR5/4-Moist); Mottles, 2.5YR48, 10-20% , 5-15mm, Prominent; Mottles, 10-
	20% ; Light clay; Strong grade of structure, 2-5 mm, Polyhedral; Smooth-ped fabric; Dry; Firm 
	consistence; 2-10%, coarse gravelly, 20-60mm, angular, Jasper, coarse fragments; , 
	Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.2); Clear change to - 
	B21	0.25 - 0.55 m	Red (2.5YR4/8-Moist); Mottles, 7.5YR64, 10-20% , 5-15mm, Prominent; Mottles, 10-20% ; Light 
	medium clay; Strong grade of structure, <2 mm, Polyhedral; Smooth-ped fabric; Dry; Firm 
	consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.5); Gradual change to - 
	B22	0.55 - 0.7 m	Red (10R4/8-Moist); Mottles, 7.5YR54, 2-10% , 5-15mm, Prominent; Mottles, 2-10% ; Light 
	medium clay; Moderate grade of structure, 5-10 mm, Subangular blocky; Smooth-ped fabric; 
	Dry; Strong consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.7); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2213	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2213	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile