Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2216	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Bright, J (Mitch)	Locality:
	Date Desc.:	21/10/93	Elevation:	No Data
	Map Ref.:	Sheet No. : 7959   GPS	Rainfall:	No Data
	Northing/Long.:	7886518 AMG zone: 55	Runoff:	Slow
	Easting/Lat.:	324094  Datum: AGD66	Drainage:	Moderately well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, No Data
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Alluvial plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	1 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Loose
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Mottled Calcic Yellow Chromosol Thin Slightly gravelly Sandy 	Principal Profile Form:	Dy5.43
	Clayey Deep
	ASC Confidence:	Great Soil Group:	Solodic soil
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Sparse. *Species includes - Chrysopogon fallax, Themeda triandra
	Mid Strata - Tree, 3.01-6m, Sparse. *Species includes - Eucalyptus platyphylla, Acacia nervosa
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - Eucalyptus platyphylla, Eucalyptus crebra, Unknown species
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.08 m	Brown (7.5YR4/2-Moist); ; Loamy sand; Single grain grade of structure; Sandy (grains 
	prominent) fabric; Dry; Very weak consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6.5 
	(Raupach, 0.05); Gradual change to - 
	A21	0.08 - 0.37 m	Light reddish brown (5YR6/4-Moist); ; Sand; Single grain grade of structure; Sandy (grains 
	prominent) fabric; Dry; Very weak consistence; 0-2%, fine gravelly, 2-6mm, rounded, coarse 
	fragments; , Calcareous, , ; , Gypseous, , ; Field pH 6.5 (Raupach, 0.2); Gradual change to - 
	A22	0.37 - 0.6 m	Light reddish brown (5YR6/4-Moist); ; Sand; Single grain grade of structure; Sandy (grains 
	prominent) fabric; Dry; Very weak consistence; 10-20%, medium gravelly, 6-20mm, rounded, 
	dispersed, coarse fragments; Few (2 - 10 %), Ferromanganiferous, Medium (2 -6 mm), 
	Nodules; , Calcareous, , ; , Gypseous, , ; Field pH 7 (Raupach, 0.5); Sharp change to - 
	B1	0.6 - 0.8 m	; Moderate grade of structure, 5-10 mm, Angular blocky; Firm consistence; , Calcareous, , ; , 
	Gypseous, , ; Ferricrete, Strongly cemented, Broken, Nodular; Clear change to - 
	B2	0.8 - 1.4 m	Light yellowish brown (10YR6/4-Moist); Mottles, 10YR74, 2-10% , 0-5mm, Prominent; Mottles, 2-
	10% ; Coarse sandy medium clay; Common (10 - 20 %), Calcareous, Coarse (6 - 20 mm), 
	Nodules; , Gypseous, , ; Field pH 8.5 (Raupach, 1); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2216	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2216	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile