Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2218	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Bright, J (Mitch)	Locality:
	Date Desc.:	22/10/93	Elevation:	No Data
	Map Ref.:	Sheet No. : 7959   GPS	Rainfall:	No Data
	Northing/Long.:	7880836 AMG zone: 55	Runoff:	Rapid
	Easting/Lat.:	327156  Datum: AGD66	Drainage:	Poorly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, No Data
	Land Form
	Rel/Slope Class: 	Undulating plains <9m 3-10%	Pattern Type:	Rises
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Very gently sloped
	Slope:	2 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Eutrophic Mottled-Subnatric Brown Sodosol Thick Non-	Principal Profile Form:	Dy2.33
	gravelly Loamy Clayey Moderately deep
	ASC Confidence:	Great Soil Group:	Solodic soil
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Very sparse. *Species includes - Bothriochloa insculpta, Chrysopogon fallax
	Mid Strata - Tree, 3.01-6m, Sparse. *Species includes - Eucalyptus crebra
	Tall Strata - Tree, 12.01-20m, Sparse. *Species includes - Eucalyptus crebra
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A11	0 - 0.08 m	Very dark greyish brown (10YR3/2-Moist); ; Sandy loam; Massive grade of structure; Earthy 
	fabric; Dry; Very weak consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6.5 (Raupach, 
	0.05); Gradual change to - 
	A12	0.08 - 0.3 m	Brown (10YR4/3-Moist); ; Sandy loam; Massive grade of structure; Earthy fabric; Dry; Weak 
	consistence; 0-2%, fine gravelly, 2-6mm, angular tabular, coarse fragments; , Calcareous, , ; , 
	Gypseous, , ; Field pH 6.5 (Raupach, 0.2); Gradual change to - 
	A2j	0.3 - 0.6 m	Yellowish brown (10YR5/8-Moist); ; Sandy clay loam (Light); Weak grade of structure, 5-10 
	mm, Polyhedral; Earthy fabric; Dry; Weak consistence; 2-10%, fine gravelly, 2-6mm, angular 
	tabular, coarse fragments; Common (10 - 20 %), Ferromanganiferous, Medium (2 -6 mm), 
	Nodules; , Calcareous, , ; , Gypseous, , ; Field pH 7 (Raupach, 0.4); 
	B2	0.6 - 1 m	Yellowish brown (10YR5/6-Moist); ; Medium clay; Strong grade of structure, 10-20 mm, 
	Prismatic; Strong grade of structure, 2-5 mm, Subangular blocky; Smooth-ped fabric; Dry; Very 
	firm consistence; Few (2 - 10 %), Manganiferous, Medium (2 -6 mm), Soft segregations; , 
	Calcareous, , ; , Gypseous, , ; Field pH 9 (Raupach, 0.7); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2218	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2218	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile