Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2236	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Rogers, Gary	Locality:
	Date Desc.:	20/10/93	Elevation:	No Data
	Map Ref.:	Sheet No. : 7957   GPS	Rainfall:	No Data
	Northing/Long.:	7872594 AMG zone: 55	Runoff:	Moderately rapid
	Easting/Lat.:	303490  Datum: AGD66	Drainage:	Well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, No Data
	Land Form
	Rel/Slope Class: 	Undulating rises 9-30m 3-10%	Pattern Type:	Rises
	Morph. Type:	Simple-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	Gently inclined
	Slope:	5 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Loose, Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Eutrophic Red Kandosol Thick Non-gravelly Loamy 	Principal Profile Form:	Gn2.12
	Clay-loamy Deep
	ASC Confidence:	Great Soil Group:	No suitable 
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Very sparse. *Species includes - Aristida species, Themeda triandra, Unknown 
	species	Mid Strata - Tree, 3.01-6m, Sparse. *Species includes - Hakea species, Grewia scabrella, Eucalyptus crebra
	Tall Strata - Tree, 6.01-12m, Mid-dense. *Species includes - Eucalyptus crebra
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.1 m	Dark brown (7.5YR3/4-Moist); ; Sandy loam; Massive grade of structure; Earthy fabric; Dry; 
	Firm consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.05); Clear change to - 
	A2	0.1 - 0.3 m	Reddish brown (5YR4/4-Moist); ; Sandy loam; Massive grade of structure; Earthy fabric; Dry; 
	Firm consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.2); Clear change to - 
	A3	0.3 - 0.8 m	Yellowish red (5YR4/6-Moist); ; Clayey sand (Heavy); Massive grade of structure; Earthy 
	fabric; Dry; Very firm consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.6); 
	Gradual change to - 
	B21	0.8 - 1.05 m	Yellowish red (5YR5/8-Moist); ; Sandy clay loam; Massive grade of structure; Earthy fabric; 
	Dry; Very firm consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.9); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2236	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2236	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile