Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2237	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Rogers, Gary	Locality:
	Date Desc.:	20/10/93	Elevation:	No Data
	Map Ref.:	Sheet No. : 7957   GPS	Rainfall:	No Data
	Northing/Long.:	7878236 AMG zone: 55	Runoff:	Rapid
	Easting/Lat.:	301062  Datum: AGD66	Drainage:	Moderately well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, No Data
	Land Form
	Rel/Slope Class: 	Undulating rises 9-30m 3-10%	Pattern Type:	Rises
	Morph. Type:	Crest	Relief:	No Data
	Elem. Type:	Hillcrest	Slope Category:	Gently inclined
	Slope:	4 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Eutrophic Mottled-Subnatric Brown Sodosol Medium Non-	Principal Profile Form:	Dy3.43
	gravelly Clay-loamy Clayey Moderately deep
	ASC Confidence:	Great Soil Group:	Solodic soil
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Very sparse. *Species includes - Unknown species, Unknown species, 
	Unknown species	Mid Strata - Tree, 1.01-3m, Very sparse. *Species includes - Eucalyptus brownii
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - Eucalyptus brownii
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.08 m	Brown (10YR4/3-Moist); ; Fine sandy clay loam (Light); Earthy fabric; Dry; Firm consistence; , 
	Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.04); Clear change to - 
	A2e	0.08 - 0.2 m	Brown (10YR5/3-Moist); ; Fine sandy clay loam (Light); Earthy fabric; Dry; Firm consistence; , 
	Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.12); Abrupt change to - 
	B21	0.2 - 0.45 m	Light olive brown (2.5Y5/4-Moist); Mottles, 2.5YR48, 10-20% , 5-15mm, Prominent; Mottles, 10-
	20% ; Sandy light medium clay; Strong grade of structure, 20-50 mm, Prismatic; Smooth-ped 
	fabric; Dry; Strong consistence; , Calcareous, , ; , Gypseous, , ; Field pH 7 (Raupach, 0.3); 
	Clear change to - 
	B22	0.45 - 0.65 m	Light olive brown (2.5Y5/6-Moist); Mottles, 2.5YR46, 2-10% , 0-5mm, Prominent; Mottles, 2-10% 
	; Sandy light clay; Moderate grade of structure, 10-20 mm, Angular blocky; Smooth-ped fabric; 
	Dry; Very firm consistence; Few (2 - 10 %), Manganiferous, Medium (2 -6 mm), Soft 
	segregations; , Calcareous, , ; , Gypseous, , ; Field pH 9.5 (Raupach, 0.6); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2237	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2237	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile