Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2251	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Rogers, Gary	Locality:
	Date Desc.:	23/08/93	Elevation:	No Data
	Map Ref.:	Sheet No. : 7859   GPS	Rainfall:	No Data
	Northing/Long.:	7890306 AMG zone: 55	Runoff:	Rapid
	Easting/Lat.:	286510  Datum: AGD66	Drainage:	Moderately well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, No Data
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  1-	Pattern Type:	Pediment
	3%
	Morph. Type:	Lower-slope	Relief:	No Data
	Elem. Type:	Footslope	Slope Category:	Very gently sloped
	Slope:	3 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Eutrophic Red Dermosol Medium Non-gravelly Clay-	Principal Profile Form:	Gn3.12
	loamy Clayey Deep
	ASC Confidence:	Great Soil Group:	No suitable 
	No analytical data are available but confidence is fair.
	Site Disturbance:	Limited clearing, for example selective logging
	Vegetation:	Low Strata - Tussock grass, 0.51-1m, Very sparse. *Species includes - None recorded
	Mid Strata - Tree, 3.01-6m, Sparse. *Species includes - Eucalyptus crebra, Eucalyptus brownii, Eremophila mitchellii
	Tall Strata - Tree, 12.01-20m, Mid-dense. *Species includes - Eucalyptus crebra, Eucalyptus brownii, Eucalyptus papuana
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A11	0 - 0.1 m	Dark brown (7.5YR3/3-Moist); ; Sandy clay loam; Massive grade of structure; Earthy fabric; 
	Dry; Very firm consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.05); Abrupt 
	change to - 
	A12	0.1 - 0.22 m	Brown (7.5YR4/4-Moist); ; Clay loam, sandy; Weak grade of structure, 5-10 mm, Polyhedral; 
	Smooth-ped fabric; Common (1-5 per 100mm2) Very fine (0.075-1mm) macropores, Dry; Very 
	firm consistence; , Calcareous, , ; , Gypseous, , ; Field pH 5.8 (Raupach, 0.15); Clear change to 
	A3	0.22 - 0.4 m	Yellowish red (5YR4/6-Moist); ; Light clay; Moderate grade of structure, 10-20 mm, Subangular 
	blocky; Smooth-ped fabric; Common (1-5 per 100mm2) Fine (1-2mm) macropores, Dry; Strong 
	consistence; 10-20%, medium gravelly, 6-20mm, subangular, Metamorphic rock (unidentified), 
	coarse fragments; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.3); Clear change to - 
	B21	0.4 - 0.75 m	Red (2.5YR4/6-Moist); ; Light clay (Heavy); Moderate grade of structure, 20-50 mm, Subangular
	 blocky; Smooth-ped fabric; Moderately moist; Very firm consistence; , Calcareous, , ; , 
	Gypseous, , ; Field pH 6 (Raupach, 0.6); Gradual change to - 
	B22	0.75 - 1.2 m	Yellowish red (5YR4/6-Moist); ; Light clay; Dry; Weak consistence; , Calcareous, , ; , 
	Gypseous, , ; Field pH 7 (Raupach, 1.1); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2251	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2251	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile