Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2264	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Rogers, Gary	Locality:
	Date Desc.:	24/08/93	Elevation:	No Data
	Map Ref.:	Sheet No. : 7859   GPS	Rainfall:	No Data
	Northing/Long.:	7877274 AMG zone: 55	Runoff:	Rapid
	Easting/Lat.:	277109  Datum: AGD66	Drainage:	Moderately well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, No Data
	Land Form
	Rel/Slope Class: 	Undulating low hills 30-90m 3-	Pattern Type:	Low hills
	10%
	Morph. Type:	Simple-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	Gently inclined
	Slope:	5 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Eutrophic Red Dermosol Thin Gravelly Clay-loamy 	Principal Profile Form:	Gn3.12
	Clayey Very shallow
	ASC Confidence:	Great Soil Group:	No suitable 
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Mid-dense. *Species includes - None recorded
	Mid Strata - Tree, 3.01-6m, Very sparse. *Species includes - Eucalyptus crebra, Eucalyptus erythrophloia
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - Eucalyptus crebra, Eucalyptus erythrophloia
	Surface Coarse Fragments:	10-20%, medium gravelly, 6-20mm, angular, 
	Profile Morphology
	A	0 - 0.05 m	Dark reddish brown (5YR3/4-Moist); ; Clay loam; Moderate grade of structure, 10-20 mm, 
	Subangular blocky; Smooth-ped fabric; Dry; Firm consistence; 2-10%, fine gravelly, 2-6mm, 
	angular, Metamorphic rock (unidentified), coarse fragments; , Calcareous, , ; , Gypseous, , ; 
	Field pH 6 (Raupach, 0.04); Clear change to - 
	B	0.05 - 0.15 m	Dark reddish brown (5YR3/4-Moist); ; Light clay; Moderate grade of structure, 10-20 mm, 
	Subangular blocky; Smooth-ped fabric; Moderately moist; Firm consistence; 10-20%, fine 
	gravelly, 2-6mm, angular, Metamorphic rock (unidentified), coarse fragments; , Calcareous, , ; , 
	Gypseous, , ; Field pH 6.5 (Raupach, 0.1); Clear change to - 
	C1	0.15 - 0.5 m	; , Calcareous, , ; , Gypseous, , ; Field pH 7 (Raupach, 0.4); 
	C2	0.5 - 1.4 m	Olive brown (2.5Y4/4-Moist); ; Sandy clay loam (Heavy); , Calcareous, , ; , Gypseous, , ; Field 
	pH 8 (Raupach, 1); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2264	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2264	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile