Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2266	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Rogers, Gary	Locality:
	Date Desc.:	24/08/93	Elevation:	No Data
	Map Ref.:	Sheet No. : 7859   GPS	Rainfall:	No Data
	Northing/Long.:	7870556 AMG zone: 55	Runoff:	Slow
	Easting/Lat.:	271176  Datum: AGD66	Drainage:	Imperfectly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, No Data
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  1-	Pattern Type:	Alluvial plain
	3%
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Very gently sloped
	Slope:	1 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Eutrophic Brown Chromosol     	Principal Profile Form:	Db1.32
	ASC Confidence:	Great Soil Group:	N/A
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.51-1m, Sparse. *Species includes - Heteropogon contortus
	Mid Strata - Tree, 6.01-12m, Very sparse. *Species includes - Eucalyptus papuana, Eucalyptus polycarpa
	Tall Strata - Tree, 12.01-20m, Sparse. *Species includes - Eucalyptus crebra, Eucalyptus papuana, Eucalyptus polycarpa
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A11	0 - 0.07 m	Dark brown (10YR3/3-Moist); ; Clayey sand; Weak grade of structure, Platy; Rough-ped fabric; 
	Dry; Weak consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.03); Clear 
	change to - 
	A12	0.07 - 0.28 m	Dark yellowish brown (10YR4/4-Moist); ; Clayey sand (Heavy); Massive grade of structure; 
	Earthy fabric; Dry; Weak consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6.5 (Raupach, 
	0.2); Clear change to - 
	A2j	0.28 - 0.5 m	Dark yellowish brown (10YR4/6-Moist); ; Sandy loam; Massive grade of structure; Earthy 
	fabric; Common (1-5 per 100mm2) Very fine (0.075-1mm) macropores, Dry; Strong 
	consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.4); Abrupt change to - 
	B21	0.5 - 0.85 m	Dark yellowish brown (10YR4/4-Moist); ; Sandy light medium clay; Moderate grade of structure,
	 20-50 mm, Subangular blocky; Smooth-ped fabric; Dry; Strong consistence; Very few (0 - 2 
	%), Manganiferous, Fine (0 - 2 mm), Soft segregations; , Calcareous, , ; , Gypseous, , ; Field pH 
	6 (Raupach, 0.6); Field pH 7 (Raupach, 0.7); Gradual change to - 
	B22	0.85 - 1 m	Dark brown (7.5YR3/2-Moist); ; Sandy light medium clay (Heavy); Strong grade of structure, 10-
	20 mm, Subangular blocky; Smooth-ped fabric; Moderately moist; Strong consistence; , 
	Calcareous, , ; , Gypseous, , ; 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2266	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2266	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile