Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2271	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Rogers, Gary	Locality:
	Date Desc.:	25/08/93	Elevation:	No Data
	Map Ref.:	Sheet No. : 7859   GPS	Rainfall:	No Data
	Northing/Long.:	7854516 AMG zone: 55	Runoff:	Rapid
	Easting/Lat.:	264631  Datum: AGD66	Drainage:	Well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, No Data
	Land Form
	Rel/Slope Class: 	Undulating low hills 30-90m 3-	Pattern Type:	Low hills
	10%
	Morph. Type:	Crest	Relief:	No Data
	Elem. Type:	Hillcrest	Slope Category:	Gently inclined
	Slope:	6 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Sodic Eutrophic Brown Chromosol Medium Gravelly Loamy 	Principal Profile Form:	Dy3.43
	Clayey Moderately deep
	ASC Confidence:	Great Soil Group:	Solodic soil
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.51-1m, Sparse. *Species includes - Aristida species, Cymbopogon bombycinus, Themeda 
	triandra	Mid Strata - Shrub, 3.01-6m, Very sparse. *Species includes - Petalostigma pubescens, Grevillea species, Eucalyptus 
	shirleyi
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - Eucalyptus brownii, Eucalyptus normantonensis, Eucalyptus 
	Surface Coarse Fragments:	10-20%, coarse gravelly, 20-60mm, angular, Sandstone
	Profile Morphology
	A1	0 - 0.03 m	Dark brown (10YR3/3-Moist); ; Sandy loam; Massive grade of structure; Earthy fabric; Dry; 
	Very firm consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.02); Abrupt 
	A2e	0.03 - 0.16 m	Yellowish brown (10YR5/4-Moist); ; Sandy loam; Massive grade of structure; Earthy fabric; 
	Dry; Strong consistence; , Calcareous, , ; , Gypseous, , ; Field pH 5.5 (Raupach, 0.1); Abrupt 
	change to - 
	B21	0.16 - 0.3 m	Yellowish brown (10YR5/4-Moist); Mottles, 10YR44, 2-10% , 0-5mm, Distinct; Mottles, 2-10% ; 
	Light medium clay; Moderate grade of structure, 20-50 mm, Prismatic; Moderate grade of 
	structure, 10-20 mm, Subangular blocky; Smooth-ped fabric; Dry; Strong consistence; , 
	Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.2); Clear change to - 
	B22	0.3 - 0.75 m	Yellowish brown (10YR5/4-Moist); Mottles, 7.5R42, 10-20% , 5-15mm, Distinct; Mottles, 10-20%
	 ; Light medium clay; Strong grade of structure, 20-50 mm, Subangular blocky; Smooth-ped 
	fabric; Dry; Strong consistence; , Calcareous, , ; , Gypseous, , ; Field pH 9 (Raupach, 0.5); Field
	 pH 9 (Raupach, 0.8); 
	R	0.75 - 1 m	Rock 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2271	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2271	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile