Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2277	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M.G. Cannon	Locality:
	Date Desc.:	01/11/93	Elevation:	No Data
	Map Ref.:	Sheet No. : 7959   GPS	Rainfall:	No Data
	Northing/Long.:	7846870 AMG zone: 55	Runoff:	Slow
	Easting/Lat.:	307119  Datum: AGD66	Drainage:	Imperfectly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  1-	Pattern Type:	Plain
	3%
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Very gently sloped
	Slope:	3 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Cracking, Self-mulching
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Self-Mulching Acidic Vertosol Slightly gravelly Fine 	Principal Profile Form:	Ug5.16
	Very fine Very deep 
	ASC Confidence:	Great Soil Group:	Black earth
	Analytical data are incomplete but reasonable confidence.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.51-1m, Sparse. *Species includes - Dichanthium species, Ophiurous exaltatus, 
	Chrysopogon fallax	Mid Strata - , , . *Species includes - None recorded
	Tall Strata - Tree, 6.01-12m, Isolated plants. *Species includes - Eucalyptus papuana, Eucalyptus crebra
	Surface Coarse Fragments:	10-20%, stony, 200-600mm, subangular, Basalt
	Profile Morphology
	A11	0 - 0.04 m	Dark brown (10YR3/3-Moist); ; Light medium clay; Strong grade of structure, 2-5 mm, Granular; 
	Strong grade of structure, <2 mm, Granular; Smooth-ped fabric; Dry; Very weak consistence; 
	Field pH 7 (Raupach, 0.02); Abrupt change to - 
	A12	0.04 - 0.3 m	Very dark grey (10YR3/1-Moist); ; Medium heavy clay; Moderate grade of structure, 50-100 
	mm, Angular blocky; Moderate grade of structure, 20-50 mm, Angular blocky; Smooth-ped 
	fabric; Dry; Rigid consistence; 0-2%, fine gravelly, 2-6mm, subangular, Quartz, coarse 
	fragments; Very few (0 - 2 %), Calcareous, Fine (0 - 2 mm), Nodules; , Gypseous, , ; Field pH 
	8.5 (Raupach, 0.2); Gradual change to - 
	B21	0.3 - 0.75 m	Very dark greyish brown (2.5Y3/2-Moist); ; Medium heavy clay; Strong grade of structure, 20-
	50 mm, Lenticular; Strong grade of structure, 5-10 mm, Angular blocky; Smooth-ped fabric; Dry; 
	Rigid consistence; Many cutans, >50% of ped faces or walls coated, distinct; Few (2 - 10 %), 
	Calcareous, Medium (2 -6 mm), Nodules; , Gypseous, , ; Field pH 8.5 (Raupach, 0.6); Gradual 
	change to - 
	B22	0.75 - 1 m	Very dark greyish brown (10YR3/2-Moist); ; Medium heavy clay; Strong grade of structure, 20-
	50 mm, Lenticular; Strong grade of structure, 2-5 mm, Angular blocky; Smooth-ped fabric; 
	Moderately moist; Strong consistence; Many cutans, >50% of ped faces or walls coated, 
	distinct; Few (2 - 10 %), Calcareous, Medium (2 -6 mm), Nodules; , Gypseous, , ; Field pH 8.5 
	(Raupach, 0.9); Gradual change to - 
	B23	1 - 1.2 m	Dark greyish brown (10YR4/2-Moist); ; Medium heavy clay; Strong grade of structure, 20-50 
	mm, Lenticular; Strong grade of structure, 2-5 mm, Angular blocky; Smooth-ped fabric; 
	Moderately moist; Strong consistence; Many cutans, >50% of ped faces or walls coated, 
	distinct; Common (10 - 20 %), Calcareous, Coarse (6 - 20 mm), Nodules; , Gypseous, , ; Field pH
	 8.5 (Raupach, 1.2); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2277	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2277	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2277	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile