Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2279	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M.G. Cannon	Locality:
	Date Desc.:	02/11/93	Elevation:	No Data
	Map Ref.:	Sheet No. : 7959   GPS	Rainfall:	No Data
	Northing/Long.:	7851930 AMG zone: 55	Runoff:	Rapid
	Easting/Lat.:	321182  Datum: AGD66	Drainage:	Moderately well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Undulating rises 9-30m 3-10%	Pattern Type:	Rises
	Morph. Type:	Upper-slope	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	Very gently sloped
	Slope:	 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Eutrophic Subnatric Brown Sodosol Thin Moderately gravelly 	Principal Profile Form:	Dy2.12
	Clay-loamy Clayey Deep
	ASC Confidence:	Great Soil Group:	No suitable 
	No analytical data are available but confidence is fair.
	Site Disturbance:	Limited clearing, for example selective logging
	Vegetation:	Low Strata - Hummock grass, 0.26-0.5m, Very sparse. *Species includes - Triodia mitchelii, Dichanthium species
	Mid Strata - Tree, 3.01-6m, Sparse. *Species includes - Eremophila mitchellii, Erythroxylon australe
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - Eucalyptus persistens, Lysiphillum carronii
	Surface Coarse Fragments:	10-20%, coarse gravelly, 20-60mm, rounded, Ironstone
	Profile Morphology
	A11	0 - 0.05 m	Dark greyish brown (10YR4/2-Moist); ; Sandy clay loam (Heavy); Massive grade of structure; 
	Earthy fabric; Dry; Weak consistence; , Calcareous, , ; , Gypseous, , ; Field pH 5.8 (Raupach, 
	0.02); 
	B1	0.05 - 0.2 m	Red (2.5YR4/6-Moist); ; Sandy clay loam (Heavy); Massive grade of structure; Earthy fabric; 
	Dry; Firm consistence; , Calcareous, , ; , Gypseous, , ; Field pH 7.5 (Raupach, 0.15); 
	B21	0.2 - 0.4 m	Yellowish brown (10YR5/8-Moist); Mottles, 7.5YR56, 2-10% , 5-15mm, Distinct; Mottles, 2-10% 
	; Light medium clay; Strong grade of structure, 10-20 mm, Subangular blocky; Strong grade of 
	structure, <2 mm, Granular; Smooth-ped fabric; Dry; Strong consistence; 10-20%, medium 
	gravelly, 6-20mm, rounded, Quartz, coarse fragments; , Calcareous, , ; , Gypseous, , ; Field pH 
	7.5 (Raupach, 0.3); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2279	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2279	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile