Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2289	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M.G. Cannon	Locality:
	Date Desc.:	03/11/93	Elevation:	No Data
	Map Ref.:	Sheet No. : 7959   GPS	Rainfall:	No Data
	Northing/Long.:	7859424 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	332790  Datum: AGD66	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, Siltstone 
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  1-	Pattern Type:	Rises
	3%
	Morph. Type:	Crest	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	Gently inclined
	Slope:	5 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Eutrophic Subnatric Grey Sodosol Medium Moderately 	Principal Profile Form:	Dy2.73
	gravelly Clay-loamy Moderately deep 
	ASC Confidence:	Great Soil Group:	Solodic soil
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Hummock grass, 0.26-0.5m, Sparse. *Species includes - TRIODIA SPECIES ?
	Mid Strata - Tree, 1.01-3m, Sparse. *Species includes - Eremophila mitchellii, Erythroxylon australe
	Tall Strata - Tree, 3.01-6m, Sparse. *Species includes - Eucalyptus persistens
	Surface Coarse Fragments:	20-50%, medium gravelly, 6-20mm, rounded, Substrate material
	Profile Morphology
	A11	0 - 0.08 m	Yellowish brown (10YR5/4-Moist); ; Sandy clay loam; Massive grade of structure; Earthy 
	fabric; Dry; Very weak consistence; , Calcareous, , ; , Gypseous, , ; Field pH 5.8 (Raupach, 
	A2j	0.08 - 0.3 m	Brown (10YR5/3-Moist); ; Sandy clay loam; Massive grade of structure; Earthy fabric; Dry; 
	Very weak consistence; , Calcareous, , ; , Gypseous, , ; Field pH 5.8 (Raupach, 0.2); 
	B21	0.3 - 0.6 m	Dark grey (10YR4/1-Moist); ; Fine sandy light clay; Massive grade of structure; Earthy fabric; 
	Dry; Very firm consistence; , Calcareous, , ; , Gypseous, , ; Field pH 9.5 (Raupach, 0.5); 
	C	0.6 - 0.8 m	; , Calcareous, , ; , Gypseous, , ; Field pH 9.5 (Raupach, 0.8); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2289	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2289	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile