Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2310	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Barry, Earl	Locality:
	Date Desc.:	11/05/94	Elevation:	No Data
	Map Ref.:	Sheet No. : 8060   GPS	Rainfall:	No Data
	Northing/Long.:	7905031 AMG zone: 55	Runoff:	Slow
	Easting/Lat.:	359665  Datum: AGD66	Drainage:	Moderately well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  1-	Pattern Type:	Alluvial plain
	3%
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Very gently sloped
	Slope:	1 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Firm
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Bleached Eutrophic Brown Chromosol Thick Non-gravelly Silty	Principal Profile Form:	Db1.43
	 Clayey Deep
	ASC Confidence:	Great Soil Group:	Brown podzolic 
	No analytical data are available but confidence is fair.	soil
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 1.01-3m, Mid-dense. *Species includes - Bothriochloa decipiens, Heteropogon contortus, 
	Chrysopogon fallax	Mid Strata - Tree, 3.01-6m, Sparse. *Species includes - Eucalyptus platyphylla
	Tall Strata - Tree, 12.01-20m, Very sparse. *Species includes - Eucalyptus platyphylla, Eucalyptus crebra, Eucalyptus 
	tessellaris
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.08 m	Very dark greyish brown (10YR3/2-Moist); ; Silty clay loam; Massive grade of structure; Dry; 
	Weak consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.05); Clear change to 
	A2e	0.08 - 0.35 m	Dark yellowish brown (10YR4/4-Moist); ; Fine sandy clay loam (Heavy); Massive grade of 
	structure; Dry; Weak consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.3); 
	Abrupt change to - 
	B21	0.35 - 0.6 m	Dark yellowish brown (10YR3/4-Moist); ; Silty heavy clay; Strong grade of structure, 20-50 mm,
	 Angular blocky; Dry; Strong consistence; , Calcareous, , ; , Gypseous, , ; Field pH 8 (Raupach, 
	0.4); Gradual change to - 
	B22	0.6 - 1 m	Brown (7.5YR4/4-Moist); ; Fine sandy medium clay; Moderate grade of structure, 10-20 mm, 
	Angular blocky; Dry; Strong consistence; , Calcareous, , ; , Gypseous, , ; Field pH 8 (Raupach, 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2310	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2310	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile