Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2319	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M.G. Cannon	Locality:
	Date Desc.:	12/05/94	Elevation:	No Data
	Map Ref.:	Sheet No. : 8060   GPS	Rainfall:	No Data
	Northing/Long.:	7934506 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	367681  Datum: AGD66	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, Igneous rock 
	(unidentified) 
	Land Form
	Rel/Slope Class: 	Gently undulating rises 9-30m  	Pattern Type:	Rises
	1-3%
	Morph. Type:	Upper-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	Gently inclined
	Slope:	10 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Soft
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Bleached-Mottled Eutrophic Grey Chromosol Medium Non-	Principal Profile Form:	Dy3.42
	gravelly Loamy Clayey Shallow
	ASC Confidence:	Great Soil Group:	Gleyed podzolic 
	No analytical data are available but confidence is fair.	soil
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Closed or dense. *Species includes - Eragrostis species, Enneapogon species, 
	Themeda triandra	Mid Strata - , , . *Species includes - None recorded
	Tall Strata - Tree, 3.01-6m, Sparse. *Species includes - Melaleuca viridiflora
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.08 m	Black (10YR2/1-Moist); ; Sandy loam; Massive grade of structure; Earthy fabric; Moderately 
	moist; Very weak consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.05); 
	A2e	0.08 - 0.18 m	Dark brown (7.5YR3/2-Moist); ; Fine sandy loam; Massive grade of structure; Earthy fabric; 
	Moderately moist; Very weak consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach,
	 0.15); 
	B1	0.18 - 0.3 m	Dark greyish brown (10YR4/2-Moist); Mottles, 10YR68, 2-10% , 5-15mm, Distinct; Mottles, 2-
	10% ; Sandy clay loam; Massive grade of structure; Earthy fabric; Moderately moist; Very weak
	 consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.25); 
	B2	0.3 - 0.45 m	Light yellowish brown (2.5Y6/4-Moist); Substrate influence, 10YR66, 10-20% , 5-15mm, 
	Distinct; Substrate influence, 10-20% ; Medium heavy clay; Strong grade of structure, 10-20 
	mm, Angular blocky; Smooth-ped fabric; Moderately moist; Very firm consistence; , Calcareous, 
	, ; , Gypseous, , ; Field pH 6 (Raupach, 0.4); 
	C	0.45 - 0.55 m	; 20-50%, medium gravelly, 6-20mm, angular, dispersed, Igneous rock (unidentified), coarse 
	fragments; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.5); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2319	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2319	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile