Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2325	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M.G. Cannon	Locality:
	Date Desc.:	13/05/94	Elevation:	No Data
	Map Ref.:	Sheet No. : 8060   GPS	Rainfall:	No Data
	Northing/Long.:	7945347 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	345060  Datum: AGD66	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Undulating rises 9-30m 3-10%	Pattern Type:	Rises
	Morph. Type:	Upper-slope	Relief:	No Data
	Elem. Type:	Fan	Slope Category:	Gently inclined
	Slope:	5 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Eutrophic Red Dermosol Medium Gravelly Clay-loamy 	Principal Profile Form:	Gn3.12
	Clayey 
	ASC Confidence:	Great Soil Group:	Red earth
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Sparse. *Species includes - Unknown species, Aristida species
	Mid Strata - Tree, 6.01-12m, Isolated plants. *Species includes - Eucalyptus crebra, Eucalyptus citriodora, Eucalyptus 
	polycarpa
	Tall Strata - Tree, 12.01-20m, Mid-dense. *Species includes - Eucalyptus crebra, Eucalyptus citriodora
	Surface Coarse Fragments:	2-10%, coarse gravelly, 20-60mm, rounded, Ferricrete
	Profile Morphology
	A	0 - 0.1 m	Dusky red (2.5YR3/2-Moist); ; Sandy clay loam; Moderate grade of structure, 2-5 mm, Granular; 
	Earthy fabric; Dry; Weak consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6.5 (Raupach, 
	0.05); 
	B1	0.1 - 0.3 m	Dark reddish brown (2.5YR3/4-Moist); ; Clay loam, sandy; Moderate grade of structure, 10-20 
	mm, Subangular blocky; Earthy fabric; Dry; Weak consistence; , Calcareous, , ; , Gypseous, , ; 
	Field pH 6.5 (Raupach, 0.2); 
	B21	0.3 - 0.5 m	Dark red (2.5YR3/6-Moist); ; Light clay; Moderate grade of structure, 10-20 mm, Subangular 
	blocky; Smooth-ped fabric; Dry; Firm consistence; Few (2 - 10 %), Argillaceous, Coarse (6 - 20 
	mm), Nodules; , Calcareous, , ; , Gypseous, , ; Field pH 7 (Raupach, 0.4); 
	B22	0.5 - 0.6 m	Dark red (10R3/6-Moist); ; Light clay; Moderate grade of structure, 10-20 mm, Subangular 
	blocky; Smooth-ped fabric; Dry; Firm consistence; Few (2 - 10 %), Argillaceous, Coarse (6 - 20 
	mm), Nodules; , Calcareous, , ; , Gypseous, , ; Field pH 7 (Raupach, 0.6); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2325	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2325	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile