Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2334	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M.G. Cannon	Locality:
	Date Desc.:	25/10/94	Elevation:	No Data
	Map Ref.:	Sheet No. : 7960   GPS	Rainfall:	No Data
	Northing/Long.:	7926620 AMG zone: 55	Runoff:	Rapid
	Easting/Lat.:	327341  Datum: AGD66	Drainage:	Moderately well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, Siltstone 
	Land Form
	Rel/Slope Class: 	Undulating rises 9-30m 3-10%	Pattern Type:	Rises
	Morph. Type:	Upper-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	Gently inclined
	Slope:	7 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 Chromosol     	Principal Profile Form:	Dy2.51
	ASC Confidence:	Great Soil Group:	No suitable 
	Confidence level not specified
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, <0.25m, Very sparse. *Species includes - Aristida species
	Mid Strata - Tree, 1.01-3m, Sparse. *Species includes - Acacia species, Bursaria incana, Erythroxylon australe
	Tall Strata - Tree, 12.01-20m, Sparse. *Species includes - Eucalyptus persistens, Eucalyptus citriodora
	Surface Coarse Fragments:	50-90%, coarse gravelly, 20-60mm, angular, Sandstone
	Profile Morphology
	A1	0 - 0.05 m	Brown (10YR4/3-Moist); ; Fine sandy loam; Massive grade of structure; Earthy fabric; Dry; Firm 
	consistence; 20-50%, medium gravelly, 6-20mm, subangular, Siltstone, coarse fragments; , 
	Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.02); Clear change to - 
	B21	0.05 - 0.25 m	Dark yellowish brown (10YR4/4-Moist); ; Silty clay loam; Massive grade of structure; Earthy 
	fabric; Dry; Very firm consistence; 2-10%, medium gravelly, 6-20mm, subangular, Siltstone, 
	coarse fragments; , Calcareous, , ; , Gypseous, , ; Field pH 5.8 (Raupach, 0.2); Clear change to 
	C	0.25 - 0.7 m	; Dry; , Calcareous, , ; , Gypseous, , ; Field pH 5.5 (Raupach, 0.6); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2334	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.05	5.9A	2B	3.3	0.32	0.11
	0.05 - 0.25	5.2A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.05
	0.05 - 0.25
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.05
	0.05 - 0.25

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2334	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	15A2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, pretreatment for 
	soluble salts
	15A2_K	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_MG	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_NA	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	4A1	pH of 1:5 soil/water suspension