Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2337	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M.G. Cannon	Locality:
	Date Desc.:	26/10/94	Elevation:	No Data
	Map Ref.:	Sheet No. : 7960   GPS	Rainfall:	No Data
	Northing/Long.:	7952736 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	319362  Datum: AGD66	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  1-	Pattern Type:	Plain
	3%
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Very gently sloped
	Slope:	1.5 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Firm
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Bleached-Ferric Mesotrophic Yellow Kandosol Medium Non-	Principal Profile Form:	Gn2.34
	gravelly Sandy Clay-loamy Moderately deep
	ASC Confidence:	Great Soil Group:	Yellow earth
	Analytical data are incomplete but reasonable confidence.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.51-1m, Sparse. *Species includes - Themeda triandra, Aristida species
	Mid Strata - Tree, 3.01-6m, Mid-dense. *Species includes - Casuarina inophloia, Grevillea glauca, Acacia species
	Tall Strata - Tree, 12.01-20m, Sparse. *Species includes - Eucalyptus polycarpa, Eucalyptus crebra
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A11	0 - 0.03 m	Dark grey (10YR4/1-Moist); ; Loamy sand; Single grain grade of structure; Sandy (grains 
	prominent) fabric; Dry; Very weak consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6.5 
	(Raupach, 0.02); 
	A12	0.03 - 0.12 m	Dark greyish brown (10YR4/2-Moist); ; Loamy sand; Massive grade of structure; Sandy (grains
	 prominent) fabric; Dry; Very weak consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6.5 
	(Raupach, 0.1); 
	A2e	0.12 - 0.38 m	Pale brown (10YR6/3-Moist); ; Loamy sand; Massive grade of structure; Sandy (grains 
	prominent) fabric; Dry; Very weak consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6.5 
	B1	0.38 - 0.5 m	Light yellowish brown (10YR6/4-Moist); ; Sandy loam; Massive grade of structure; Earthy 
	fabric; Dry; Very weak consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6.5 (Raupach, 
	B21	0.5 - 0.8 m	Brownish yellow (10YR6/8-Moist); ; Sandy clay loam; Massive grade of structure; Earthy 
	fabric; Dry; Very weak consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6.5 (Raupach, 
	0.6); Field pH 6.5 (Raupach, 0.8); 
	B22c	0.8 - 0.9 m	Brownish yellow (10YR6/8-Moist); ; Sandy clay loam; Massive grade of structure; Earthy 
	fabric; Dry; Very weak consistence; Many (20 - 50 %), Ferruginous, Medium (2 -6 mm), 
	Nodules; , Calcareous, , ; , Gypseous, , ; 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2337	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.03	6A	1.6B	0.66	0.18	0.05
	0.03 - 0.12	6.1A
	0.12 - 0.38	6.2A
	0.38 - 0.5	6.4A
	0.5 - 0.8	6.2A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.03
	0.03 - 0.12
	0.12 - 0.38
	0.38 - 0.5
	0.5 - 0.8
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.03
	0.03 - 0.12
	0.12 - 0.38
	0.38 - 0.5
	0.5 - 0.8

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2337	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	15A2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, pretreatment for 
	soluble salts
	15A2_K	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_MG	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_NA	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	4A1	pH of 1:5 soil/water suspension