Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2343	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M.G. Cannon	Locality:
	Date Desc.:	26/10/94	Elevation:	No Data
	Map Ref.:	Sheet No. : 7960   GPS	Rainfall:	No Data
	Northing/Long.:	7918576 AMG zone: 55	Runoff:	Rapid
	Easting/Lat.:	292743  Datum: AGD66	Drainage:	Well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Undulating rises 9-30m 3-10%	Pattern Type:	Rises
	Morph. Type:	Mid-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	Gently inclined
	Slope:	7 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Eutrophic Red Dermosol Medium Slightly gravelly Sandy	Principal Profile Form:	Gn3
	 Clayey Moderately deep
	ASC Confidence:	Great Soil Group:	Red earth
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Sparse. *Species includes - Themeda triandra
	Mid Strata - Tree, 3.01-6m, Very sparse. *Species includes - Petalostigma pubescens, Grevillea parallela, Acacia species
	Tall Strata - Tree, 12.01-20m, Sparse. *Species includes - Eucalyptus polycarpa, Erthrophleum chlorostachys, Eucalyptus 
	melanophloia
	Surface Coarse Fragments:	2-10%, medium gravelly, 6-20mm, subangular, Quartz
	Profile Morphology
	A11	0 - 0.03 m	; Loamy fine sand; Massive grade of structure; Earthy fabric; Dry; Very weak consistence; , 
	Calcareous, , ; , Gypseous, , ; Clear change to - 
	A2	0.03 - 0.25 m	; Fine sandy loam; Massive grade of structure; Earthy fabric; Dry; Very weak consistence; , 
	Calcareous, , ; , Gypseous, , ; Diffuse change to - 
	B2	0.25 - 0.6 m	; Medium clay; Moderate grade of structure, 10-20 mm, Subangular blocky; Smooth-ped fabric; 
	Dry; Very firm consistence; 0-2%, fine gravelly, 2-6mm, rounded, dispersed, Detrital 
	sedimentary rock (unidentified), coarse fragments; , Calcareous, , ; , Gypseous, , ; 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2343	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.03	6.1A	3.9B	1.5	0.47	0.08
	0.25 - 0.6	5.8A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.03
	0.25 - 0.6
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.03
	0.25 - 0.6

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2343	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	15A2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, pretreatment for 
	soluble salts
	15A2_K	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_MG	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_NA	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	4A1	pH of 1:5 soil/water suspension