Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2346	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M.G. Cannon	Locality:
	Date Desc.:	27/10/94	Elevation:	No Data
	Map Ref.:	Sheet No. : 7860   GPS	Rainfall:	No Data
	Northing/Long.:	7949844 AMG zone: 55	Runoff:	Slow
	Easting/Lat.:	262711  Datum: AGD66	Drainage:	Moderately well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  1-	Pattern Type:	Plain
	3%
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Very gently sloped
	Slope:	2 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Firm
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Eutrophic Brown Ferrosol Medium Non-gravelly Clay-	Principal Profile Form:	Gn3.22
	loamy Clayey Moderately deep
	ASC Confidence:	Great Soil Group:	Euchrozem
	Analytical data are incomplete but reasonable confidence.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.51-1m, Mid-dense. *Species includes - Themeda triandra, Heteropogon contortus, 
	Heteropogon triticeus	Mid Strata - , , . *Species includes - None recorded
	Tall Strata - Tree, 12.01-20m, Very sparse. *Species includes - Eucalyptus crebra, Eucalyptus papuana
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A11	0 - 0.12 m	Dark brown (10YR3/3-Moist); ; Clay loam; Strong grade of structure, 2-5 mm, Granular; Dry; 
	Weak consistence; Very few (0 - 2 %), Manganiferous, Fine (0 - 2 mm), Nodules; , Calcareous, 
	, ; , Gypseous, , ; Field pH 6 (Raupach, 0.05); 
	B1	0.12 - 0.3 m	Brown (7.5YR4/4-Moist); ; Light clay; Strong grade of structure, 5-10 mm, Angular blocky; Dry; 
	Weak consistence; Very few (0 - 2 %), Manganiferous, Fine (0 - 2 mm), Nodules; , Calcareous, 
	, ; , Gypseous, , ; Field pH 6 (Raupach, 0.3); 
	B21	0.3 - 0.9 m	Brown (10YR4/3-Moist); ; Medium heavy clay; Strong grade of structure, 20-50 mm, Lenticular; 
	Strong grade of structure, 5-10 mm, Angular blocky; Moderately moist; Firm consistence; Many 
	cutans, >50% of ped faces or walls coated; Few (2 - 10 %), Manganiferous, Fine (0 - 2 mm), 
	Nodules; , Calcareous, , ; , Gypseous, , ; Field pH 7 (Raupach, 0.9); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2346	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.12	6.2A	16B	12	1.5	0.16
	0.12 - 0.3	6.5A
	0.3 - 0.9	7.3A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.12
	0.12 - 0.3
	0.3 - 0.9
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.12
	0.12 - 0.3
	0.3 - 0.9

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2346	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	15A2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, pretreatment for 
	soluble salts
	15A2_K	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_MG	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_NA	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	4A1	pH of 1:5 soil/water suspension