Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2354	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Rogers, Gary	Locality:
	Date Desc.:	25/10/94	Elevation:	No Data
	Map Ref.:	Sheet No. : 7960   GPS	Rainfall:	No Data
	Northing/Long.:	7928412 AMG zone: 55	Runoff:	Moderately rapid
	Easting/Lat.:	324783  Datum: AGD66	Drainage:	Moderately well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Undulating rises 9-30m 3-10%	Pattern Type:	Rises
	Morph. Type:	Upper-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	Gently inclined
	Slope:	5 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Mesotrophic Red Chromosol Thick Slightly gravelly 	Principal Profile Form:	Dr2.51
	Sandy Clayey Moderately deep
	ASC Confidence:	Great Soil Group:	No suitable 
	Confidence level not specified
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Sparse. *Species includes - Heteropogon contortus, Themeda triandra
	Mid Strata - Tree, 3.01-6m, Very sparse. *Species includes - Eucalyptus crebra
	Tall Strata - Tree, 12.01-20m, Sparse. *Species includes - Eucalyptus crebra, Eucalyptus papuana
	Surface Coarse Fragments:	2-10%, medium gravelly, 6-20mm, angular, Quartz
	Profile Morphology
	A11	0 - 0.05 m	Very dark greyish brown (10YR3/2-Moist); ; Loamy sand; Massive grade of structure; Sandy 
	(grains prominent) fabric; Dry; 20-50%, fine gravelly, 2-6mm, angular, Quartz, coarse 
	fragments; , Calcareous, , ; , Gypseous, , ; Field pH 6.5 (Raupach, 0.03); Abrupt change to - 
	A12	0.05 - 0.13 m	Dark yellowish brown (10YR4/4-Moist); ; Clayey sand (Light); Massive grade of structure; 
	Sandy (grains prominent) fabric; Dry; 20-50%, medium gravelly, 6-20mm, angular, Quartz, 
	coarse fragments; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.1); Clear change to - 
	A13	0.13 - 0.45 m	Dark yellowish brown (10YR4/6-Moist); ; Clayey sand (Light); Massive grade of structure; 
	Sandy (grains prominent) fabric; Dry; 20-50%, fine gravelly, 2-6mm, angular, Quartz, coarse 
	fragments; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.3); Abrupt change to - 
	B3	0.45 - 0.5 m	Red (2.5YR4/8-Moist); ; Light medium clay; Massive grade of structure; Sandy (grains 
	prominent) fabric; Dry; 2-10%, fine gravelly, 2-6mm, angular, Quartz, coarse fragments; , 
	Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.5); 
	R	0.5 - 0.7 m	Rock 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2354	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2354	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile