Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2355	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Rogers, Gary	Locality:
	Date Desc.:	25/10/94	Elevation:	No Data
	Map Ref.:	Sheet No. : 7960   GPS	Rainfall:	No Data
	Northing/Long.:	7934277 AMG zone: 55	Runoff:	Rapid
	Easting/Lat.:	317628  Datum: AGD66	Drainage:	Imperfectly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Undulating rises 9-30m 3-10%	Pattern Type:	Rises
	Morph. Type:	Simple-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	Gently inclined
	Slope:	3 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Eutrophic Red Dermosol Medium Non-gravelly Clay-	Principal Profile Form:	Dr2.13
	loamy Clayey Moderately deep
	ASC Confidence:	Great Soil Group:	Red podzolic soil
	Confidence level not specified
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, <0.25m, Isolated plants. *Species includes - None recorded
	Mid Strata - , , . *Species includes - None recorded
	Tall Strata - Tree, 6.01-12m, Mid-dense. *Species includes - Eucalyptus persistens
	Surface Coarse Fragments:	0-2%, fine gravelly, 2-6mm, subangular, 
	Profile Morphology
	A1	0 - 0.1 m	Dark yellowish brown (10YR3/6-Moist); ; Sandy clay loam; Massive grade of structure; Earthy 
	fabric; Dry; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.05); Clear change to - 
	B21	0.1 - 0.4 m	Yellowish red (5YR4/6-Moist); ; Silty light clay; Moderate grade of structure, 20-50 mm; Smooth-
	ped fabric; Dry; Very few (0 - 2 %), Manganiferous, Fine (0 - 2 mm), Tubules; , Calcareous, , ; , 
	Gypseous, , ; Field pH 6.5 (Raupach, 0.3); Clear change to - 
	B22	0.4 - 0.6 m	Strong brown (7.5YR5/6-Moist); ; Silty light clay; Moderate grade of structure, 10-20 mm; 
	Smooth-ped fabric; Dry; 2-10%, coarse gravelly, 20-60mm, angular, Substrate material, coarse 
	fragments; Very few (0 - 2 %), Manganiferous, Fine (0 - 2 mm), Tubules; , Calcareous, , ; , 
	Gypseous, , ; Soil matrix is Highly calcareous; Field pH 8.5 (Raupach, 0.6); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2355	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0.01 - 0.1	4.9A	3.3B	4.2	0.13	1.7
	0.1 - 0.4	4.9A
	0.4 - 0.5	9.1A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0.01 - 0.1
	0.1 - 0.4
	0.4 - 0.5
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0.01 - 0.1
	0.1 - 0.4
	0.4 - 0.5

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2355	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	15A2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, pretreatment for 
	soluble salts
	15A2_K	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_MG	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_NA	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	4A1	pH of 1:5 soil/water suspension