Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2366	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Rogers, Gary	Locality:
	Date Desc.:	27/10/94	Elevation:	No Data
	Map Ref.:	Sheet No. : 7860   GPS	Rainfall:	No Data
	Northing/Long.:	7922450 AMG zone: 55	Runoff:	Rapid
	Easting/Lat.:	273517  Datum: AGD66	Drainage:	Imperfectly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  1-	Pattern Type:	Plain
	3%
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Very gently sloped
	Slope:	2 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Eutrophic Brown Kandosol Thick Slightly gravelly Clay-	Principal Profile Form:	Gn2.23
	loamy Clayey Deep
	ASC Confidence:	Great Soil Group:	No suitable 
	Confidence level not specified
	Site Disturbance:	Limited clearing, for example selective logging
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Isolated plants. *Species includes - None recorded
	Mid Strata - Tree, 1.01-3m, Isolated plants. *Species includes - Bursaria incana
	Tall Strata - Tree, 12.01-20m, Very sparse. *Species includes - Eucalyptus brownii, Eucalyptus papuana, Eucalyptus 
	Surface Coarse Fragments:	2-10%, medium gravelly, 6-20mm, subangular, Quartz
	Profile Morphology
	A11	0 - 0.03 m	Dark brown (10YR3/3-Moist); ; Sandy clay loam (Heavy); Moderate grade of structure, 10-20 
	mm, Platy; Rough-ped fabric; Dry; 0-2%, fine gravelly, 2-6mm, subrounded, Quartz, coarse 
	fragments; Very few (0 - 2 %), Manganiferous, Fine (0 - 2 mm), Nodules; , Calcareous, , ; , 
	Gypseous, , ; Field pH 6 (Raupach, 0.02); Clear change to - 
	A12	0.03 - 0.15 m	Dark yellowish brown (10YR4/4-Moist); ; Clay loam, sandy; Massive grade of structure; Earthy 
	fabric; Dry; 0-2%, fine gravelly, 2-6mm, subrounded, Quartz, coarse fragments; , Calcareous, , 
	; , Gypseous, , ; Field pH 5.5 (Raupach, 0.1); Clear change to - 
	A13	0.15 - 0.4 m	Dark yellowish brown (10YR4/6-Moist); ; Light clay; Weak grade of structure, 10-20 mm, 
	Subangular blocky; Smooth-ped fabric; Dry; 2-10%, fine gravelly, 2-6mm, subrounded, Quartz, 
	coarse fragments; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.3); Clear change to - 
	B21	0.4 - 0.8 m	Brown (10YR4/3-Moist); ; Medium clay; Moderate grade of structure, 20-50 mm, Subangular 
	blocky; Smooth-ped fabric; Dry; 2-10%, fine gravelly, 2-6mm, subrounded, Quartz, coarse 
	fragments; Few (2 - 10 %), Manganiferous, Medium (2 -6 mm), Nodules; , Calcareous, , ; , 
	Gypseous, , ; Field pH 7 (Raupach, 0.6); Gradual change to - 
	B22	0.8 - 1.1 m	Dark yellowish brown (10YR4/4-Moist); ; Medium clay; Dry; Few (2 - 10 %), Manganiferous, 
	Medium (2 -6 mm), Nodules; , Calcareous, , ; , Gypseous, , ; Field pH 8.5 (Raupach, 1); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2366	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0.03 - 0.15	5.1A	2.3B	4.3	0.31	0.34
	0.15 - 0.4	6A
	0.4 - 0.8	7.7A
	0.8 - 1.1	8.6A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0.03 - 0.15
	0.15 - 0.4
	0.4 - 0.8
	0.8 - 1.1
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0.03 - 0.15
	0.15 - 0.4
	0.4 - 0.8
	0.8 - 1.1

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2366	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	15A2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, pretreatment for 
	soluble salts
	15A2_K	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_MG	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_NA	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	4A1	pH of 1:5 soil/water suspension