Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2367	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Rogers, Gary	Locality:
	Date Desc.:	27/10/94	Elevation:	No Data
	Map Ref.:	Sheet No. : 7860   GPS	Rainfall:	No Data
	Northing/Long.:	7922506 AMG zone: 55	Runoff:	Very slow
	Easting/Lat.:	273516  Datum: AGD66	Drainage:	Imperfectly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  1-	Pattern Type:	Plain
	3%
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Very gently sloped
	Slope:	2 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Cracking, Self-mulching
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Mottled Self-Mulching Black Vertosol Non-gravelly Medium 	Principal Profile Form:	Ug5.25
	fine Very fine Deep 
	ASC Confidence:	Great Soil Group:	Grey clay
	Confidence level not specified
	Site Disturbance:	Limited clearing, for example selective logging
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Isolated plants. *Species includes - Unknown species, Unknown species, 
	Unknown species	Mid Strata - Tree, 1.01-3m, Isolated plants. *Species includes - Bursaria incana
	Tall Strata - Tree, 12.01-20m, Very sparse. *Species includes - Eucalyptus brownii, Eucalyptus papuana, Eucalyptus 
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.05 m	Olive brown (2.5Y4/4-Moist); ; Light clay; Strong grade of structure, 2-5 mm, Granular; Smooth-
	ped fabric; Dry; 0-2%, fine gravelly, 2-6mm, subrounded, Quartz, coarse fragments; , 
	Calcareous, , ; , Gypseous, , ; Field pH 7 (Raupach, 0.03); Clear change to - 
	B21	0.05 - 0.35 m	Dark greyish brown (2.5Y4/2-Moist); Mottles, 10YR34, 2-10% , 5-15mm, Faint; Mottles, 2-10% ; 
	Light medium clay; Strong grade of structure, 20-50 mm, Subangular blocky; Smooth-ped fabric;
	 Dry; 2-10%, fine gravelly, 2-6mm, subrounded, Quartz, coarse fragments; , Calcareous, , ; , 
	Gypseous, , ; Field pH 7 (Raupach, 0.2); Clear change to - 
	B22	0.35 - 0.7 m	Dark brown (10YR3/3-Moist); ; Medium clay; Moderate grade of structure, 20-50 mm, Angular 
	blocky; Smooth-ped fabric; Dry; 0-2%, fine gravelly, 2-6mm, subrounded, Quartz, coarse 
	fragments; , Calcareous, , ; , Gypseous, , ; Field pH 7 (Raupach, 0.6); Gradual change to - 
	B23	0.7 - 1.2 m	Dark greyish brown (2.5Y4/2-Moist); Mottles, 10YR56, 0-2% , 0-5mm, Faint; Mottles, 0-2% ; 
	Medium heavy clay; Dry; 0-2%, fine gravelly, 2-6mm, subrounded, Quartz, coarse fragments; , 
	Calcareous, , ; , Gypseous, , ; Field pH 7.5 (Raupach, 1.1); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2367	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.05	6.8A	13B	14	0.68	0.47
	0.05 - 0.35	7.1A
	0.35 - 0.7	7.4A
	0.7 - 1.2	8.3A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.05
	0.05 - 0.35
	0.35 - 0.7
	0.7 - 1.2
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.05
	0.05 - 0.35
	0.35 - 0.7
	0.7 - 1.2

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2367	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	15A2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, pretreatment for 
	soluble salts
	15A2_K	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_MG	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_NA	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	4A1	pH of 1:5 soil/water suspension