Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2376	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M.G. Cannon	Locality:
	Date Desc.:	27/10/94	Elevation:	No Data
	Map Ref.:	Sheet No. : 7860   GPS	Rainfall:	No Data
	Northing/Long.:	7898749 AMG zone: 55	Runoff:	Moderately rapid
	Easting/Lat.:	272141  Datum: AGD66	Drainage:	Moderately well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  1-	Pattern Type:	Plain
	3%
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Very gently sloped
	Slope:	4 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Eutrophic Yellow Ferrosol Thin Non-gravelly Loamy 	Principal Profile Form:	Um
	Loamy Moderately deep
	ASC Confidence:	Great Soil Group:	Xanthozem
	No analytical data are available but confidence is fair.
	Site Disturbance:	Highly disturbed, for example, quarrying, roadworks, mining, landfill, urban
	Vegetation:	Low Strata - Tussock grass, 0.51-1m, Very sparse. *Species includes - Chrysopogon fallax, Aristida species
	Mid Strata - , , . *Species includes - None recorded
	Tall Strata - Tree, 12.01-20m, Sparse. *Species includes - Eucalyptus crebra
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.08 m	Dark brown (10YR3/3-Moist); ; Clay loam; Massive grade of structure; Earthy fabric; Dry; Very 
	weak consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6.5 (Raupach, 0.05); 
	A3	0.08 - 0.3 m	Brown (7.5YR4/4-Moist); ; Clay loam; Massive grade of structure; Earthy fabric; Dry; Very 
	weak consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6.2 (Raupach, 0.25); 
	B2	0.3 - 0.6 m	Brownish yellow (10YR6/8-Moist); ; Clay loam (Heavy); Strong grade of structure, 10-20 mm, 
	Subangular blocky; Strong grade of structure, 2-5 mm, Subangular blocky; Smooth-ped fabric; 
	Dry; Weak consistence; 0-2%, medium gravelly, 6-20mm, subangular, dispersed, Quartz, 
	coarse fragments; , Calcareous, , ; , Gypseous, , ; 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2376	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.08	6.1A	7.6B	3.2	0.87	0.08
	0.3 - 0.6	5.6A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.08
	0.3 - 0.6
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.08
	0.3 - 0.6

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2376	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	15A2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, pretreatment for 
	soluble salts
	15A2_K	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_MG	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_NA	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	4A1	pH of 1:5 soil/water suspension