Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	24	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M. DeCorte	Locality:
	Date Desc.:	27/06/90	Elevation:	200 metres
	Map Ref.:	Sheet No. : 8356   GPS	Rainfall:	No Data
	Northing/Long.:	7718575 AMG zone: 55	Runoff:	Very rapid
	Easting/Lat.:	515482  Datum: AGD66	Drainage:	Well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Existing vertical exposure, Igneous rock 
	(unidentified) 
	Land Form
	Rel/Slope Class: 	Rolling hills 90-300m 10-32%	Pattern Type:	Hills
	Morph. Type:	Mid-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	Moderately inclined
	Slope:	22 % 	Aspect:	300 degrees
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Eutrophic Brown Chromosol Thin Very gravelly Clay-	Principal Profile Form:	Db1.12
	loamy Clayey Shallow
	ASC Confidence:	Great Soil Group:	No suitable 
	Analytical data are incomplete but reasonable confidence.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - , , . *Species includes - Bothriochloa bladhii, Chrysopogon fallax, Aristida species
	Mid Strata - , , . *Species includes - Eucalyptus crebra, Eucalyptus erythrophloia, Acacia species
	Tall Strata - Tree, 12.01-20m, Sparse. *Species includes - Eucalyptus crebra, Eucalyptus erythrophloia, Eucalyptus 
	Surface Coarse Fragments:	50-90%, cobbly, 60-200mm, angular, Substrate material
	Profile Morphology
	A1	0 - 0.08 m	Yellowish brown (10YR5/4-Moist); ; Sandy clay loam (Light); Weak grade of structure, 5-10 
	mm, Subangular blocky; Earthy fabric; Dry; Very weak consistence; , Calcareous, , ; , 
	Gypseous, , ; Field pH 7 (Raupach, 0.05); Common, fine (1-2mm) roots; Clear, Smooth change to
	B2	0.08 - 0.25 m	Dark yellowish brown (10YR4/6-Moist); ; Light clay; Moderate grade of structure, 10-20 mm, 
	Subangular blocky; Moderate grade of structure, 2-5 mm, Subangular blocky; Smooth-ped 
	fabric; Moderately moist; Very weak consistence; , Calcareous, , ; , Gypseous, , ; Field pH 7.5 
	(Raupach, 0.2); Few, very fine (0-1mm) roots; Clear, Smooth change to - 
	BC	0.25 - 0.35 m	; , Calcareous, , ; , Gypseous, , ; 
	R	0.35 - 1.2 m	Rock 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	24	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.08	9A	10B	3	0.28	0.16
	0.08 - 0.25	8.7A	13.4J	3.5	0.2	0.3	18.1I	1.66
	0.35 - 1.2	8.8A	11E	2.9	0.04	0.24	13B	1.85
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.08
	0.08 - 0.25
	0.35 - 1.2
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.08
	0.08 - 0.25
	0.35 - 1.2

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	24	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	10B	Extractable sulfur(mg/kg) - Phosphate extractable sulfur
	15A2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, pretreatment for 
	soluble salts
	15A2_K	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_MG	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_NA	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15C1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - alcoholic 1M ammonium chloride at pH 8.5, pretreatment 
	for soluble salts
	15C1_CEC	CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble salts
	15C1_K	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble 
	salts
	15C1_MG	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble 
	salts
	15C1_NA	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble 
	salts
	15F1_CA	Exchangeable bases by 0.01M silver-thiourea (AgTU)+, no pretreatment for soluble salts
	15F1_K	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_MG	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_NA	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F3	CEC by 0.01M silver-thiourea (AgTU)+
	15N1	Exchangeable sodium percentage (ESP)
	4A1	pH of 1:5 soil/water suspension