Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2405	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Rogers, Gary	Locality:
	Date Desc.:	10/05/94	Elevation:	No Data
	Map Ref.:	Sheet No. : 8060   GPS	Rainfall:	No Data
	Northing/Long.:	7908972 AMG zone: 55	Runoff:	Moderately rapid
	Easting/Lat.:	368883  Datum: AGD66	Drainage:	Well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Undulating rises 9-30m 3-10%	Pattern Type:	Low hills
	Morph. Type:	Crest	Relief:	No Data
	Elem. Type:	Hillcrest	Slope Category:	Gently inclined
	Slope:	8 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Firm, Soft
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Eutrophic Brown Kandosol Thick Non-gravelly Sandy 	Principal Profile Form:	Gn2
	Clayey Moderately deep
	ASC Confidence:	Great Soil Group:	Yellow earth
	No analytical data are available but confidence is fair.
	Site Disturbance:	Limited clearing, for example selective logging
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Very sparse. *Species includes - Heteropogon contortus, Aristida species, 
	Eragrostis species	Mid Strata - Tree, 3.01-6m, Very sparse. *Species includes - Eucalyptus crebra
	Tall Strata - , , . *Species includes - Eucalyptus crebra, Eucalyptus papuana, Eucalyptus tessellaris
	Surface Coarse Fragments:	50-90%, fine gravelly, 2-6mm, angular, Granite
	Profile Morphology
	A11	0 - 0.1 m	Dark brown (10YR3/3-Moist); ; Loamy coarse sand; Massive grade of structure; Earthy fabric; 
	Dry; 2-10%, fine gravelly, 2-6mm, angular, Quartz, coarse fragments; , Calcareous, , ; , 
	Gypseous, , ; Field pH 6.5 (Raupach, 0.05); Clear change to - 
	A12	0.1 - 0.25 m	Brown (10YR4/3-Moist); ; Clayey coarse sand; Massive grade of structure; Earthy fabric; Dry; 
	2-10%, fine gravelly, 2-6mm, angular, Quartz, coarse fragments; , Calcareous, , ; , Gypseous, , 
	; Field pH 6.5 (Raupach, 0.2); Abrupt change to - 
	A13	0.25 - 0.55 m	Dark yellowish brown (10YR4/6-Moist); ; Clayey coarse sand; Massive grade of structure; 
	Earthy fabric; Dry; 20-50%, fine gravelly, 2-6mm, angular, Quartz, coarse fragments; , 
	Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.4); Clear change to - 
	B1	0.55 - 0.7 m	Yellowish brown (10YR5/6-Moist); ; Coarse sandy clay loam (Heavy); Massive grade of 
	structure; Earthy fabric; Dry; 50-90%, medium gravelly, 6-20mm, angular, Quartz, coarse 
	fragments; , Calcareous, , ; , Gypseous, , ; Field pH 6.5 (Raupach, 0.6); Abrupt change to - 
	B2	0.7 - 0.8 m	Light olive brown (2.5Y5/6-Moist); ; Coarse sandy clay loam; Dry; 20-50%, fine gravelly, 2-6mm,
	 angular, Quartz, coarse fragments; , Calcareous, , ; , Gypseous, , ; Field pH 7 (Raupach, 0.8); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2405	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2405	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile