Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2430	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	Rogers, Gary	Locality:
	Date Desc.:	12/01/94	Elevation:	No Data
	Map Ref.:	Sheet No. : 8158   GPS	Rainfall:	No Data
	Northing/Long.:	7799570 AMG zone: 55	Runoff:	Very slow
	Easting/Lat.:	417160  Datum: AGD66	Drainage:	Moderately well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, No Data
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Alluvial plain
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Terrace flat	Slope Category:	Level
	Slope:	1 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Bleached-Sodic Eutrophic Black Dermosol Thick Non-gravelly 	Principal Profile Form:	Dd3.32
	Clay-loamy Clayey Deep
	ASC Confidence:	Great Soil Group:	Brown earth
	Analytical data are incomplete but reasonable confidence.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Sparse. *Species includes - Bothriochloa ewartiana, Chrysopogon fallax, 
	Dichanthium species	Mid Strata - Tree, 3.01-6m, Very sparse. *Species includes - Eucalyptus species, Atalaya hemiglauca, Pleiogynium 
	cerasiferum
	Tall Strata - Tree, 12.01-20m, Sparse. *Species includes - Eucalyptus crebra, Eucalyptus brownii
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.2 m	Very dark grey (10YR3/1-Moist); ; Clay loam, fine sandy; Massive grade of structure; Earthy 
	fabric; Moist; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.1); Clear change to - 
	A2e	0.2 - 0.4 m	Dark greyish brown (10YR4/2-Moist); ; Clay loam, fine sandy; Massive grade of structure; 
	Earthy fabric; Moderately moist; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.3); 
	Abrupt change to - 
	B21	0.4 - 0.9 m	Very dark grey (10YR3/1-Moist); ; Fine sandy light medium clay; Moderate grade of structure, 
	20-50 mm, Prismatic; Smooth-ped fabric; Dry; , Calcareous, , ; , Gypseous, , ; Field pH 7 
	(Raupach, 0.6); Gradual change to - 
	B22	0.9 - 1.2 m	Very dark greyish brown (10YR3/2-Moist); ; Medium clay; Moderate grade of structure, 20-50 
	mm, Subangular blocky; Smooth-ped fabric; Dry; Very few (0 - 2 %), Calcareous, Fine (0 - 2 
	mm), Nodules; , Gypseous, , ; Soil matrix is Slightly calcareous; Field pH 8.5 (Raupach, 1.1); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2430	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	2430	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile