Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	262	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M. DeCorte	Locality:
	Date Desc.:	19/06/91	Elevation:	260 metres
	Map Ref.:	Sheet No. : 8157   GPS	Rainfall:	No Data
	Northing/Long.:	7779690 AMG zone: 55	Runoff:	Rapid
	Easting/Lat.:	434591  Datum: AGD66	Drainage:	Well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, Granulite 
	Land Form
	Rel/Slope Class: 	Gently undulating rises 9-30m  	Pattern Type:	Rises
	1-3%
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	1 % 	Aspect:	80 degrees
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Eutrophic Mesonatric Black Sodosol Medium Moderately 	Principal Profile Form:	Dd1.43
	gravelly Clay-loamy Clayey Moderately deep
	ASC Confidence:	Great Soil Group:	Solodized 
	All necessary analytical data are available.	solonetz
	Site Disturbance:	Extensive clearing, for example poisoning, ringbarking
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Very sparse. *Species includes - Aristida species, Eragrostis species
	Mid Strata - Tree, 3.01-6m, Sparse. *Species includes - Eremophila mitchellii
	Tall Strata - Tree, 6.01-12m, Mid-dense. *Species includes - Eucalyptus brownii
	Surface Coarse Fragments:	20-50%, coarse gravelly, 20-60mm, angular, Quartz
	Profile Morphology
	A11	0 - 0.06 m	Brown (10YR4/3-Moist); ; Coarse sandy clay loam; Massive grade of structure; Earthy fabric; 
	Common (1-5 per 100mm2) Fine (1-2mm) macropores, Dry; Weak consistence; , Calcareous, , ; 
	, Gypseous, , ; Abrupt, Smooth change to - 
	A12	0.06 - 0.12 m	Dark brown (10YR3/3-Moist); ; Coarse sandy loam (Heavy); Massive grade of structure; Earthy
	 fabric; Common (1-5 per 100mm2) Fine (1-2mm) macropores, Dry; Weak consistence; , 
	Calcareous, , ; , Gypseous, , ; Abrupt, Smooth change to - 
	A2e	0.12 - 0.14 m	Dark brown (10YR3/3-Moist); ; Coarse sandy loam (Heavy); Massive grade of structure; Earthy
	 fabric; Common (1-5 per 100mm2) Very fine (0.075-1mm) macropores, Dry; Firm consistence; ,
	 Calcareous, , ; , Gypseous, , ; Abrupt, Smooth change to - 
	B21	0.14 - 0.55 m	Very dark greyish brown (10YR3/2-Moist); ; Coarse sandy light clay; Strong grade of structure,
	 20-50 mm, Columnar; Strong grade of structure, 10-20 mm, Angular blocky; Smooth-ped fabric; 
	Common (1-5 per 100mm2) Very fine (0.075-1mm) macropores, Moderately moist; Very firm 
	consistence; 0-2%, fine gravelly, 2-6mm, angular, dispersed, Quartz, coarse fragments; , 
	Calcareous, , ; , Gypseous, , ; Gradual, Smooth change to - 
	C	0.55 - 0.65 m	; , Calcareous, , ; , Gypseous, , ; 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	262	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.06	6.3A
	0.14 - 0.55	8.3A	6.7J	10.1	0.1	3.2	15.9I	20.13
	0.55 - 0.65	8.8A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.06
	0.14 - 0.55
	0.55 - 0.65
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.06
	0.14 - 0.55
	0.55 - 0.65

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	262	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	15F1_CA	Exchangeable bases by 0.01M silver-thiourea (AgTU)+, no pretreatment for soluble salts
	15F1_K	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_MG	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_NA	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F3	CEC by 0.01M silver-thiourea (AgTU)+
	15N1	Exchangeable sodium percentage (ESP)
	4A1	pH of 1:5 soil/water suspension