Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	266	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M. DeCorte	Locality:
	Date Desc.:	10/06/91	Elevation:	300 metres
	Map Ref.:	Sheet No. : 8157   GPS	Rainfall:	No Data
	Northing/Long.:	7777782 AMG zone: 55	Runoff:	Very slow
	Easting/Lat.:	427540  Datum: AGD66	Drainage:	Well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, Granodiorite 
	Land Form
	Rel/Slope Class: 	Undulating rises 9-30m 3-10%	Pattern Type:	Rises
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	1 % 	Aspect:	270 degrees
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Eutrophic Red Chromosol Medium Non-gravelly Sandy 	Principal Profile Form:	Dr2.22
	Clayey Moderately deep
	ASC Confidence:	Great Soil Group:	Non-calcic brown
	Analytical data are incomplete but reasonable confidence.	 soil
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.51-1m, Sparse. *Species includes - Heteropogon contortus, Chrysopogon fallax, 
	Bothriochloa ewartiana	Mid Strata - Tree, 1.01-3m, Sparse. *Species includes - Acacia bidwillii, Eucalyptus erythrophloia, Acacia bidwillii
	Tall Strata - Tree, 3.01-6m, Very sparse. *Species includes - Eucalyptus erythrophloia, Eucalyptus papuana, Eucalyptus 
	melanophloia
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A11	0 - 0.08 m	Dark brown (10YR3/3-Moist); ; Loamy sand; Massive grade of structure; Earthy fabric; Many 
	(>5 per 100mm2) Fine (1-2mm) macropores, Dry; Very weak consistence; , Calcareous, , ; , 
	Gypseous, , ; Field pH 5.5 (Raupach, 0.05); Common, very fine (0-1mm) roots; Abrupt, Smooth 
	change to - 
	A12	0.08 - 0.12 m	Brown (7.5YR4/4-Moist); ; Loamy coarse sand; Massive grade of structure; Earthy fabric; 
	Many (>5 per 100mm2) Fine (1-2mm) macropores, Dry; Weak consistence; , Calcareous, , ; , 
	Gypseous, , ; Common, very fine (0-1mm) roots; Abrupt, Smooth change to - 
	B1	0.12 - 0.25 m	Dark red (2.5YR3/6-Moist); ; Light clay; Strong grade of structure, 20-50 mm, Angular blocky; 
	Strong grade of structure, 5-10 mm, Angular blocky; Smooth-ped fabric; Few (<1 per 100mm2) 
	Very fine (0.075-1mm) macropores, Dry; Firm consistence; , Calcareous, , ; , Gypseous, , ; 
	Few, very fine (0-1mm) roots; Clear, Smooth change to - 
	B2	0.25 - 0.62 m	Red (2.5YR4/6-Moist); ; Light clay; Strong grade of structure, 20-50 mm, Angular blocky; Strong
	 grade of structure, 5-10 mm, Angular blocky; Smooth-ped fabric; Few (<1 per 100mm2) Very 
	fine (0.075-1mm) macropores, Moderately moist; Very firm consistence; 0-2%, medium gravelly,
	 6-20mm, angular, dispersed, Granodiorite, coarse fragments; Common cutans, 10-50% of ped 
	faces or walls coated, distinct; , Calcareous, , ; , Gypseous, , ; Field pH 7.5 (Raupach, 0.6); 
	Few, very fine (0-1mm) roots; 
	C	0.62 - 0.85 m	; , Calcareous, , ; , Gypseous, , ; 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	266	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.08	5.8A
	0.25 - 0.62	6.6A	9.6J	2.8	0.6	0.1	12.7I	0.79
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.08
	0.25 - 0.62
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.08
	0.25 - 0.62

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	266	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	15F1_CA	Exchangeable bases by 0.01M silver-thiourea (AgTU)+, no pretreatment for soluble salts
	15F1_K	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_MG	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_NA	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F3	CEC by 0.01M silver-thiourea (AgTU)+
	15N1	Exchangeable sodium percentage (ESP)
	4A1	pH of 1:5 soil/water suspension