Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	280	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M. DeCorte	Locality:
	Date Desc.:	20/06/91	Elevation:	320 metres
	Map Ref.:	Sheet No. : 8257   GPS	Rainfall:	No Data
	Northing/Long.:	7754658 AMG zone: 55	Runoff:	Very slow
	Easting/Lat.:	451515  Datum: AGD66	Drainage:	Well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, Gabbro 
	Land Form
	Rel/Slope Class: 	Undulating rises 9-30m 3-10%	Pattern Type:	Rises
	Morph. Type:	Lower-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	Gently inclined
	Slope:	4 % 	Aspect:	290 degrees
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Eutrophic Red Chromosol Medium Non-gravelly Loamy 	Principal Profile Form:	Dr2.13
	Clayey Moderately deep
	ASC Confidence:	Great Soil Group:	Non-calcic brown
	All necessary analytical data are available.	 soil
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.51-1m, Mid-dense. *Species includes - Heteropogon contortus, Bothriochloa pertusa, 
	Bothriochloa decipiens	Mid Strata - Tree, 1.01-3m, Very sparse. *Species includes - Eucalyptus erythrophloia
	Tall Strata - Tree, 6.01-12m, Very sparse. *Species includes - Eucalyptus crebra, Eucalyptus erythrophloia
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A11	0 - 0.02 m	Very dark brown (10YR2/2-Moist); ; Loam; Massive grade of structure; Earthy fabric; Many (>5 
	per 100mm2) Medium (2-5mm) macropores, Dry; Very weak consistence; , Calcareous, , ; , 
	Gypseous, , ; Common, fine (1-2mm) roots; Clear, Smooth change to - 
	A12	0.02 - 0.12 m	Dark brown (7.5YR3/2-Moist); ; Loamy fine sand (Heavy); Massive grade of structure; Earthy 
	fabric; Many (>5 per 100mm2) Medium (2-5mm) macropores, Dry; Weak consistence; , 
	Calcareous, , ; , Gypseous, , ; Field pH 6.5 (Raupach, 0.05); Common, fine (1-2mm) roots; 
	Gradual, Smooth change to - 
	B1	0.12 - 0.28 m	Dark reddish brown (5YR3/4-Moist); ; Sandy clay loam; Weak grade of structure, 10-20 mm, 
	Subangular blocky; Smooth-ped fabric; Many (>5 per 100mm2) Fine (1-2mm) macropores, 
	Moderately moist; Weak consistence; , Calcareous, , ; , Gypseous, , ; Common, very fine (0-
	1mm) roots; Clear, Smooth change to - 
	B21	0.28 - 0.65 m	Reddish brown (5YR4/4-Moist); ; Medium clay (Heavy); Moderate grade of structure, 10-20 mm,
	 Subangular blocky; Smooth-ped fabric; Many (>5 per 100mm2) Fine (1-2mm) macropores, 
	Moderately moist; Very firm consistence; Many cutans, >50% of ped faces or walls coated, 
	distinct; , Calcareous, , ; , Gypseous, , ; Field pH 8.5 (Raupach, 0.6); Common, very fine (0-
	1mm) roots; Abrupt, Smooth change to - 
	C	0.65 - 0.7 m	; , Calcareous, , ; , Gypseous, , ; 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	280	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0.02 - 0.12	6.5A
	0.28 - 0.65	7.5A	13.3J	5.9	0.1	0.3	15.5I	1.94
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0.02 - 0.12
	0.28 - 0.65
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0.02 - 0.12
	0.28 - 0.65

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	280	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	15F1_CA	Exchangeable bases by 0.01M silver-thiourea (AgTU)+, no pretreatment for soluble salts
	15F1_K	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_MG	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_NA	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F3	CEC by 0.01M silver-thiourea (AgTU)+
	15N1	Exchangeable sodium percentage (ESP)
	4A1	pH of 1:5 soil/water suspension