Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	282	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M. DeCorte	Locality:
	Date Desc.:	20/06/91	Elevation:	340 metres
	Map Ref.:	Sheet No. : 8157   GPS	Rainfall:	No Data
	Northing/Long.:	7753208 AMG zone: 55	Runoff:	Very slow
	Easting/Lat.:	447604  Datum: AGD66	Drainage:	Moderately well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, Ferricrete 
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	1 % 	Aspect:	0 degrees
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Mesotrophic Yellow Kandosol Thin Non-gravelly Loamy	Principal Profile Form:	Gn2.32
	 Clay-loamy Moderately deep
	ASC Confidence:	Great Soil Group:	Yellow earth
	Analytical data are incomplete but reasonable confidence.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Sparse. *Species includes - Chrysopogon fallax, Eragrostis species, Aristida 
	Mid Strata - Tree, 1.01-3m, Very sparse. *Species includes - Petalostigma pubescens, Eucalyptus crebra, Melaleuca 
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - Eucalyptus crebra, Eucalyptus polycarpa
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.07 m	Very dark greyish brown (10YR3/2-Moist); ; Loam; Massive grade of structure; Earthy fabric; 
	Many (>5 per 100mm2) Fine (1-2mm) macropores, Dry; Weak consistence; , Calcareous, , ; , 
	Gypseous, , ; Field pH 6 (Raupach, 0.05); Common, fine (1-2mm) roots; Clear, Smooth change to
	 - 
	A2j	0.07 - 0.2 m	Brown (10YR5/3-Moist); Mottles, 7.5YR56, 10-20% , 0-5mm, Distinct; Mottles, 10-20% ; Sandy 
	clay loam; Massive grade of structure; Earthy fabric; Many (>5 per 100mm2) Fine (1-2mm) 
	macropores, Dry; Weak consistence; , Calcareous, , ; , Gypseous, , ; Common, fine (1-2mm) 
	roots; Clear, Smooth change to - 
	B21	0.2 - 0.52 m	Brownish yellow (10YR6/6-Moist); Mottles, 7.5YR56, 0-2% , 0-5mm, Distinct; Mottles, 0-2% ; 
	Clay loam; Massive grade of structure; Earthy fabric; Many (>5 per 100mm2) Fine (1-2mm) 
	macropores, Moderately moist; Weak consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6 
	(Raupach, 0.3); Abrupt, Smooth change to - 
	B22c	0.52 - 0.8 m	; Earthy fabric;  Fine (1-2mm) macropores, , Calcareous, , ; , Gypseous, , ; Ferricrete, 
	Uncemented, Continuous, Massive; Field pH 6.5 (Raupach, 0.6); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	282	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.07	6.2A
	0.2 - 0.52	6.1A	2.8J	1.7	0.1	0.2	1.1I	18.18
	0.52 - 0.8	6.3A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.07
	0.2 - 0.52
	0.52 - 0.8
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.07
	0.2 - 0.52
	0.52 - 0.8

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	282	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	15F1_CA	Exchangeable bases by 0.01M silver-thiourea (AgTU)+, no pretreatment for soluble salts
	15F1_K	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_MG	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_NA	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F3	CEC by 0.01M silver-thiourea (AgTU)+
	15N1	Exchangeable sodium percentage (ESP)
	4A1	pH of 1:5 soil/water suspension