Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	297	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M. DeCorte	Locality:
	Date Desc.:	03/07/91	Elevation:	290 metres
	Map Ref.:	Sheet No. : 8257   GPS	Rainfall:	No Data
	Northing/Long.:	7743104 AMG zone: 55	Runoff:	Very slow
	Easting/Lat.:	465226  Datum: AGD66	Drainage:	Well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  1-	Pattern Type:	Plain
	3%
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Very gently sloped
	Slope:	1 % 	Aspect:	80 degrees
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Sodic Eutrophic Red Sodosol Medium Non-gravelly Sandy 	Principal Profile Form:	Dr2.22
	Clayey Moderately deep
	ASC Confidence:	Great Soil Group:	Non-calcic brown
	Analytical data are incomplete but reasonable confidence.	 soil
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Sparse. *Species includes - Bothriochloa decipiens, Chrysopogon fallax, 
	Eragrostis species	Mid Strata - Tree, 3.01-6m, Isolated plants. *Species includes - Eucalyptus crebra
	Tall Strata - Tree, 6.01-12m, Mid-dense. *Species includes - None Recorded
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.05 m	Dark reddish brown (5YR3/4-Moist); ; Loamy fine sand; Massive grade of structure; Earthy 
	fabric; Dry; Firm consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.05); 
	Common, fine (1-2mm) roots; Abrupt, Smooth change to - 
	A3	0.05 - 0.25 m	Yellowish red (5YR4/6-Moist); ; Clay loam, fine sandy; Massive grade of structure; Earthy 
	fabric; Dry; Firm consistence; , Calcareous, , ; , Gypseous, , ; Common, very fine (0-1mm) roots;
	 Gradual, Smooth change to - 
	B1	0.25 - 0.48 m	Yellowish red (5YR5/6-Moist); ; Fine sandy light clay; Weak grade of structure, 20-50 mm, 
	Subangular blocky; Smooth-ped fabric; Dry; Firm consistence; , Calcareous, , ; , Gypseous, , ; 
	Field pH 6 (Raupach, 0.3); Common, very fine (0-1mm) roots; Clear, Smooth change to - 
	B21	0.48 - 0.7 m	Yellowish red (5YR5/6-Moist); ; Light medium clay; Strong grade of structure, 5-10 mm, 
	Subangular blocky; Smooth-ped fabric; Moderately moist; Strong consistence; 0-2%, medium 
	gravelly, 6-20mm, subrounded, Metamorphic rock (unidentified), coarse fragments; , 
	Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.6); Common, very fine (0-1mm) roots; 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	297	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.05	5.8A
	0.25 - 0.48	5.9A
	0.48 - 0.7	6.4A	2.3J	2.1	0.4	0.3	7.6I	3.95
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.05
	0.25 - 0.48
	0.48 - 0.7
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.05
	0.25 - 0.48
	0.48 - 0.7

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	297	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	15F1_CA	Exchangeable bases by 0.01M silver-thiourea (AgTU)+, no pretreatment for soluble salts
	15F1_K	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_MG	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_NA	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F3	CEC by 0.01M silver-thiourea (AgTU)+
	15N1	Exchangeable sodium percentage (ESP)
	4A1	pH of 1:5 soil/water suspension