Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	299	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M. DeCorte	Locality:
	Date Desc.:	03/07/91	Elevation:	280 metres
	Map Ref.:	Sheet No. : 8257   GPS	Rainfall:	No Data
	Northing/Long.:	7739910 AMG zone: 55	Runoff:	Slow
	Easting/Lat.:	467810  Datum: AGD66	Drainage:	Imperfectly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Gently undulating rises 9-30m  	Pattern Type:	Rises
	1-3%
	Morph. Type:	Mid-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	Very gently sloped
	Slope:	2 % 	Aspect:	90 degrees
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Bleached-Mottled Mesotrophic Grey Chromosol Medium Non-	Principal Profile Form:	Dy2.42
	gravelly Sandy Clayey Moderately deep
	ASC Confidence:	Great Soil Group:	No suitable 
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Very sparse. *Species includes - Chrysopogon fallax, Aristida species
	Mid Strata - Shrub, 0.51-1m, Isolated plants. *Species includes - Erythroxylon australe
	Tall Strata - Tree, 6.01-12m, Very sparse. *Species includes - Eucalyptus brownii
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.05 m	Dark grey (5Y4/1-Moist); ; Coarse sand; Massive grade of structure; Earthy fabric; Dry; Firm 
	consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6.5 (Raupach, 0.05); Clear, Smooth 
	change to - 
	A2e	0.05 - 0.22 m	Dark grey (7.5YR4/0-Moist); ; Coarse sand; Massive grade of structure; Earthy fabric; Dry; Firm
	 consistence; , Calcareous, , ; , Gypseous, , ; Abrupt, Tongued change to - 
	B21	0.22 - 0.5 m	Dark grey (7.5YR4/0-Moist); Mottles, 7.5YR58, 10-20% , 0-5mm, Distinct; Mottles, 10-20% ; 
	Coarse sandy light clay; Strong grade of structure, 10-20 mm, Angular blocky; Smooth-ped 
	fabric; Dry; Strong consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.3); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	299	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	299	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile