Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	30	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M. DeCorte	Locality:
	Date Desc.:	28/06/90	Elevation:	170 metres
	Map Ref.:	Sheet No. : 8257   GPS	Rainfall:	No Data
	Northing/Long.:	7740250 AMG zone: 55	Runoff:	Moderately rapid
	Easting/Lat.:	496672  Datum: AGD66	Drainage:	Well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Auger boring, Granodiorite 
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  1-	Pattern Type:	Plain
	3%
	Morph. Type:	Upper-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	Very gently sloped
	Slope:	2 % 	Aspect:	270 degrees
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Pedal Hypercalcic Calcarosol Non-gravelly Clayey 	Principal Profile Form:	Uf6.34
	Clayey Shallow 
	ASC Confidence:	Great Soil Group:	No suitable 
	All necessary analytical data are available.
	Site Disturbance:	Limited clearing, for example selective logging
	Vegetation:	Low Strata - , , . *Species includes - Bothriochloa pertusa, Bothriochloa bladhii, Chrysopogon fallax
	Mid Strata - , , . *Species includes - Eucalyptus erythrophloia
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - Eucalyptus erythrophloia, Eucalyptus crebra, Eucalyptus 
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.15 m	Dark brown (10YR3/3-Moist); ; Light medium clay; Moderate grade of structure, 20-50 mm, 
	Angular blocky; Earthy fabric; Moderately moist; Weak consistence; Field pH 7.8 (Raupach, 
	0.05); Few, very fine (0-1mm) roots; Abrupt, Smooth change to - 
	B21	0.15 - 0.3 m	Dark yellowish brown (10YR3/4-Moist); ; Light clay; Moderate grade of structure, 20-50 mm, 
	Angular blocky; Earthy fabric; Moderately moist; Weak consistence; 2-10%, coarse gravelly, 
	20-60mm, angular, dispersed, Igneous rock (unidentified), coarse fragments; Soil matrix is Very 
	highly calcareous; Field pH 8.5 (Raupach, 0.3); Few, very fine (0-1mm) roots; Clear, Smooth 
	change to - 
	Ck	0.3 - 1 m	Yellowish brown (10YR5/6-Moist); ; Clay loam; Massive grade of structure; Earthy fabric; 
	Moderately moist; Very weak consistence; 2-10%, coarse gravelly, 20-60mm, angular, 
	dispersed, Igneous rock (unidentified), coarse fragments; Very many (50 - 100 %), Calcareous,
	 Coarse (6 - 20 mm), Soft segregations; , Gypseous, , ; Soil matrix is Very highly calcareous; 
	Field pH 8.5 (Raupach, 0.6); 
	2Ck	1 - 1.05 m	; Massive grade of structure; Earthy fabric; Moderately moist; Very weak consistence; Many 
	(20 - 50 %), Calcareous, Coarse (6 - 20 mm), Soft segregations; , Gypseous, , ; Soil matrix is 
	Very highly calcareous; Field pH 8.8 (Raupach, 1.05); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	30	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.15	8.6A	24B	3.1	0.64	0.05
	0.15 - 0.3	9.1A	20E	1.8	0.18	0.63	20B	3.15
	23.7J	1.5	0.1	0.3	22.5I	2.80
	1.50
	1.33
	0.3 - 1	9.5A
	1 - 1.05	9.7A	32B	2	0.06	0.18
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.15
	0.15 - 0.3
	0.3 - 1
	1 - 1.05
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.15
	0.15 - 0.3
	0.3 - 1
	1 - 1.05

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	30	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	10B	Extractable sulfur(mg/kg) - Phosphate extractable sulfur
	15A2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, pretreatment for 
	soluble salts
	15A2_K	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_MG	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_NA	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15C1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - alcoholic 1M ammonium chloride at pH 8.5, pretreatment 
	for soluble salts
	15C1_CEC	CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble salts
	15C1_K	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble 
	salts
	15C1_MG	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble 
	salts
	15C1_NA	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble 
	salts
	15F1_CA	Exchangeable bases by 0.01M silver-thiourea (AgTU)+, no pretreatment for soluble salts
	15F1_K	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_MG	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_NA	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F3	CEC by 0.01M silver-thiourea (AgTU)+
	15N1	Exchangeable sodium percentage (ESP)
	4A1	pH of 1:5 soil/water suspension