Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	31	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M. DeCorte	Locality:
	Date Desc.:	28/06/90	Elevation:	170 metres
	Map Ref.:	Sheet No. : 8257   GPS	Rainfall:	No Data
	Northing/Long.:	7740860 AMG zone: 55	Runoff:	Moderately rapid
	Easting/Lat.:	498403  Datum: AGD66	Drainage:	Well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Auger boring, Granodiorite 
	Land Form
	Rel/Slope Class: 	Undulating rises 9-30m 3-10%	Pattern Type:	Rises
	Morph. Type:	Crest	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	Gently inclined
	Slope:	5 % 	Aspect:	240 degrees
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Eutrophic Red Kandosol Medium Non-gravelly Clay-	Principal Profile Form:	Gn2.12
	loamy Clay-loamy Shallow
	ASC Confidence:	Great Soil Group:	Red earth
	All necessary analytical data are available.
	Site Disturbance:	Extensive clearing, for example poisoning, ringbarking
	Vegetation:	Low Strata - , , . *Species includes - Bothriochloa pertusa, Bothriochloa bladhii
	Mid Strata - , , . *Species includes - Eucalyptus erythrophloia
	Tall Strata - Tree, 6.01-12m, Very sparse. *Species includes - Eucalyptus erythrophloia, Eucalyptus crebra, Eucalyptus 
	papuana
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.1 m	Dark brown (7.5YR3/4-Moist); ; Sandy clay loam (Light); Weak grade of structure, 10-20 mm, 
	Subangular blocky; Smooth-ped fabric; Dry; Firm consistence; , Calcareous, , ; , Gypseous, , ; 
	Field pH 6.5 (Raupach, 0.05); Few, very fine (0-1mm) roots; Clear, Smooth change to - 
	B21	0.1 - 0.3 m	Yellowish red (5YR4/6-Moist); ; Clay loam, sandy; Weak grade of structure, 10-20 mm, 
	Subangular blocky; Smooth-ped fabric; Moderately moist; Weak consistence; , Calcareous, , ; , 
	Gypseous, , ; Field pH 6.8 (Raupach, 0.3); Few, very fine (0-1mm) roots; Clear, Smooth change 
	to - 
	C	0.3 - 0.6 m	; Massive grade of structure; Moderately moist; Weak consistence; , Calcareous, , ; , 
	Gypseous, , ; Field pH 7.5 (Raupach, 0.6); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	31	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	8A	6.3B	2.8	0.33	0.06
	0.1 - 0.3	8A	11J	3.3	0.1	0.6	14.1I	4.26
	0.3 - 0.6	8.3A	10B	3.3	0.09	0.12
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1
	0.1 - 0.3
	0.3 - 0.6
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.3
	0.3 - 0.6

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	31	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	10B	Extractable sulfur(mg/kg) - Phosphate extractable sulfur
	15A2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, pretreatment for 
	soluble salts
	15A2_K	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_MG	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_NA	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15F1_CA	Exchangeable bases by 0.01M silver-thiourea (AgTU)+, no pretreatment for soluble salts
	15F1_K	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_MG	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_NA	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F3	CEC by 0.01M silver-thiourea (AgTU)+
	15N1	Exchangeable sodium percentage (ESP)
	4A1	pH of 1:5 soil/water suspension