Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	333	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M. DeCorte	Locality:
	Date Desc.:	30/07/91	Elevation:	320 metres
	Map Ref.:	Sheet No. : 8157   GPS	Rainfall:	No Data
	Northing/Long.:	7755554 AMG zone: 55	Runoff:	Slow
	Easting/Lat.:	434661  Datum: AGD66	Drainage:	Well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, Granodiorite 
	Land Form
	Rel/Slope Class: 	Undulating rises 9-30m 3-10%	Pattern Type:	Rises
	Morph. Type:	Upper-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	Gently inclined
	Slope:	3 % 	Aspect:	270 degrees
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Eutrophic Red Chromosol Medium Non-gravelly Sandy 	Principal Profile Form:	Dr2.12
	Clayey Shallow
	ASC Confidence:	Great Soil Group:	Non-calcic brown
	No analytical data are available but confidence is fair.	 soil
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.51-1m, Mid-dense. *Species includes - Chrysopogon fallax, Heteropogon contortus, 
	Aristida species	Mid Strata - Tree, 3.01-6m, Isolated plants. *Species includes - Eucalyptus erythrophloia, Acacia bidwillii
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - Eucalyptus crebra, Eucalyptus erythrophloia, Eucalyptus 
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.08 m	Dark brown (7.5YR3/3-Moist); ; Coarse sand; Weak grade of structure, 10-20 mm, Subangular 
	blocky; Smooth-ped fabric; Dry; Firm consistence; 2-10%, fine gravelly, 2-6mm, angular, 
	dispersed, Granodiorite, coarse fragments; , Calcareous, , ; , Gypseous, , ; Field pH 6.5 
	(Raupach, 0.05); Clear, Smooth change to - 
	A3	0.08 - 0.18 m	Reddish brown (5YR4/4-Moist); ; Coarse sand; Weak grade of structure, 10-20 mm, Subangular
	 blocky; Smooth-ped fabric; Dry; Very firm consistence; 2-10%, fine gravelly, 2-6mm, angular, 
	dispersed, Granodiorite, coarse fragments; , Calcareous, , ; , Gypseous, , ; Abrupt, Smooth 
	change to - 
	B21	0.18 - 0.4 m	Dark reddish brown (2.5YR3/4-Moist); ; Medium clay; Strong grade of structure, 20-50 mm, 
	Angular blocky; Smooth-ped fabric; Dry; Strong consistence; 0-2%, fine gravelly, 2-6mm, 
	angular, dispersed, Granodiorite, coarse fragments; , Calcareous, , ; , Gypseous, , ; Field pH 7 
	(Raupach, 0.3); Clear, Smooth change to - 
	B/C	0.4 - 0.5 m	Dark red (2.5YR3/8-Moist); Substrate influence, 5YR58, 10-20% , 5-15mm, Prominent; Substrate
	 influence, 10-20% ; Light clay; Strong grade of structure, 10-20 mm, Angular blocky; Smooth-
	ped fabric; Dry; Strong consistence; 2-10%, medium gravelly, 6-20mm, angular, dispersed, 
	Granodiorite, coarse fragments; , Calcareous, , ; , Gypseous, , ; 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	333	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	333	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile