Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	337	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M. DeCorte	Locality:
	Date Desc.:	30/07/91	Elevation:	340 metres
	Map Ref.:	Sheet No. : 8157   GPS	Rainfall:	No Data
	Northing/Long.:	7741959 AMG zone: 55	Runoff:	Very rapid
	Easting/Lat.:	430706  Datum: AGD66	Drainage:	Well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Existing vertical exposure, Rhyolite 
	Land Form
	Rel/Slope Class: 	Undulating rises 9-30m 3-10%	Pattern Type:	Rises
	Morph. Type:	Mid-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	Gently inclined
	Slope:	6 % 	Aspect:	20 degrees
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Eutrophic Red Chromosol Thin Very gravelly Loamy 	Principal Profile Form:	Dr2.13
	Clayey Moderately deep
	ASC Confidence:	Great Soil Group:	Non-calcic brown
	All necessary analytical data are available.	 soil
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Very sparse. *Species includes - Chrysopogon fallax, Aristida species
	Mid Strata - Tree, 1.01-3m, Sparse. *Species includes - Eremophila mitchellii, Atalaya hemiglauca
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - Eucalyptus brownii
	Surface Coarse Fragments:	50-90%, coarse gravelly, 20-60mm, subrounded, Rhyolite
	Profile Morphology
	A1	0 - 0.03 m	Dark reddish brown (5YR3/3-Moist); ; Sandy loam; Weak grade of structure, 5-10 mm, 
	Subangular blocky; Smooth-ped fabric; Dry; Strong consistence; 50-90%, medium gravelly, 6-
	20mm, subrounded, dispersed, Rhyolite, coarse fragments; , Calcareous, , ; , Gypseous, , ; 
	Abrupt, Smooth change to - 
	B1	0.03 - 0.12 m	Dark reddish brown (5YR3/4-Moist); ; Light clay; Strong grade of structure, 10-20 mm, Angular 
	blocky; Smooth-ped fabric; Dry; Very strong consistence; 2-10%, medium gravelly, 6-20mm, 
	subrounded, dispersed, Rhyolite, coarse fragments; , Calcareous, , ; , Gypseous, , ; Field pH 6 
	(Raupach, 0.05); Clear, Smooth change to - 
	B21	0.12 - 0.5 m	Reddish brown (5YR4/4-Moist); ; Medium clay; Strong grade of structure, 10-20 mm, Angular 
	blocky; Smooth-ped fabric; Dry; Very strong consistence; , Calcareous, , ; , Gypseous, , ; Field 
	pH 8 (Raupach, 0.3); Clear, Smooth change to - 
	B22	0.5 - 0.7 m	Yellowish red (5YR4/6-Moist); ; Medium clay; Strong grade of structure, 10-20 mm, Angular 
	blocky; Smooth-ped fabric; Dry; Very strong consistence; , Calcareous, , ; , Gypseous, , ; Field 
	pH 9.5 (Raupach, 0.6); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	337	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0.03 - 0.12	6.5A	12B	3.8	0.19	0.11
	0.12 - 0.5	7.4A
	0.5 - 0.7	8.1A	29B	5.3	0.05	0.07	16.3I	0.43
	13.9J	4.3	0	0.1	0.61
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0.03 - 0.12
	0.12 - 0.5
	0.5 - 0.7
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0.03 - 0.12
	0.12 - 0.5
	0.5 - 0.7

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	337	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	10B	Extractable sulfur(mg/kg) - Phosphate extractable sulfur
	15A2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, pretreatment for 
	soluble salts
	15A2_K	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_MG	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_NA	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15F1_CA	Exchangeable bases by 0.01M silver-thiourea (AgTU)+, no pretreatment for soluble salts
	15F1_K	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_MG	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_NA	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F3	CEC by 0.01M silver-thiourea (AgTU)+
	15N1	Exchangeable sodium percentage (ESP)
	4A1	pH of 1:5 soil/water suspension