Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	339	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M. DeCorte	Locality:
	Date Desc.:	30/07/91	Elevation:	320 metres
	Map Ref.:	Sheet No. : 8157   GPS	Rainfall:	No Data
	Northing/Long.:	7741200 AMG zone: 55	Runoff:	No Data
	Easting/Lat.:	434622  Datum: AGD66	Drainage:	Moderately well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Gently undulating rises 9-30m  	Pattern Type:	Rises
	1-3%
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Gently inclined
	Slope:	3 % 	Aspect:	290 degrees
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Basic Ferric Orthic Tenosol Thin Non-gravelly Sandy Loamy 	Principal Profile Form:	Uc5.22
	Moderately deep
	ASC Confidence:	Great Soil Group:	Earthy sand
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.26-0.5m, Very sparse. *Species includes - Aristida species, Chrysopogon fallax
	Mid Strata - Tree, 3.01-6m, Sparse. *Species includes - Eucalyptus crebra
	Tall Strata - Tree, 12.01-20m, Very sparse. *Species includes - Eucalyptus crebra
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.07 m	Brown (7.5YR4/4-Moist); ; Loamy sand; Massive grade of structure; Earthy fabric; Dry; Very 
	weak consistence; Few (2 - 10 %), Ferromanganiferous, Coarse (6 - 20 mm), Nodules; , 
	Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.05); Clear, Smooth change to - 
	A3	0.07 - 0.4 m	Strong brown (7.5YR5/6-Moist); ; Loamy sand; Massive grade of structure; Earthy fabric; Dry; 
	Very weak consistence; Many (20 - 50 %), Ferromanganiferous, Very coarse (20 - 60 mm), 
	Nodules; , Calcareous, , ; , Gypseous, , ; Field pH 6.5 (Raupach, 0.3); Gradual, Smooth change 
	to - 
	B21c	0.4 - 0.6 m	Strong brown (7.5YR5/6-Moist); ; Coarse sandy loam (Heavy); Massive grade of structure; 
	Earthy fabric; Dry; Very weak consistence; 0-2%, medium gravelly, 6-20mm, angular, 
	dispersed, Rhyolite, coarse fragments; , Calcareous, , ; , Gypseous, , ; Field pH 7.5 (Raupach, 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	339	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	339	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile