Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	350	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M. DeCorte	Locality:
	Date Desc.:	01/08/91	Elevation:	380 metres
	Map Ref.:	Sheet No. : 8157   GPS	Rainfall:	No Data
	Northing/Long.:	7753506 AMG zone: 55	Runoff:	Slow
	Easting/Lat.:	409893  Datum: AGD66	Drainage:	Imperfectly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Undulating rises 9-30m 3-10%	Pattern Type:	Rises
	Morph. Type:	Mid-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	Gently inclined
	Slope:	2.5 % 	Aspect:	0 degrees
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Eutrophic Mottled-Subnatric Brown Sodosol Thick Non-	Principal Profile Form:	Dy3.43
	gravelly Sandy Clayey Moderately deep
	ASC Confidence:	Great Soil Group:	Solodized 
	No analytical data are available but confidence is fair.	solonetz
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.51-1m, Mid-dense. *Species includes - Chrysopogon fallax, Heteropogon contortus, 
	Bothriochloa pertusa	Mid Strata - Tree, 1.01-3m, Sparse. *Species includes - Eucalyptus crebra
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - Eucalyptus crebra, Eucalyptus brownii, Eucalyptus papuana
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.1 m	Dark brown (10YR3/3-Moist); ; Coarse sand; Massive grade of structure; Sandy (grains 
	prominent) fabric; Dry; Weak consistence; 2-10%, fine gravelly, 2-6mm, subrounded, dispersed,
	 Quartz, coarse fragments; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.05); Gradual,
	 Smooth change to - 
	A21	0.1 - 0.35 m	Brown (7.5YR5/4-Moist); ; Coarse sand; Massive grade of structure; Sandy (grains prominent) 
	fabric; Dry; Weak consistence; 10-20%, fine gravelly, 2-6mm, subrounded, dispersed, Quartz, 
	coarse fragments; , Calcareous, , ; , Gypseous, , ; Field pH 7 (Raupach, 0.3); Clear, Smooth 
	change to - 
	A22e	0.35 - 0.37 m	Very pale brown (10YR7/4-Moist); ; Coarse sand; Massive grade of structure; Sandy (grains 
	prominent) fabric; Dry; Weak consistence; 20-50%, fine gravelly, 2-6mm, subrounded, 
	dispersed, Quartz, coarse fragments; , Calcareous, , ; , Gypseous, , ; Abrupt, Smooth change 
	B21	0.37 - 0.65 m	Yellowish brown (10YR5/6-Moist); Mottles, 5YR58, 20-50% , 0-5mm, Prominent; Mottles, 
	10YR54, 20-50% ; Medium clay; Strong grade of structure, 20-50 mm, Columnar; Strong grade 
	of structure, 10-20 mm, Angular blocky; Smooth-ped fabric; Dry; Strong consistence; 10-20%, 
	fine gravelly, 2-6mm, subrounded, dispersed, Quartz, coarse fragments; , Calcareous, , ; , 
	Gypseous, , ; Field pH 7.5 (Raupach, 0.6); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	350	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0.37 - 0.65	7.9A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0.37 - 0.65
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0.37 - 0.65

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	350	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	4A1	pH of 1:5 soil/water suspension