Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	364	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M. DeCorte	Locality:
	Date Desc.:	12/08/91	Elevation:	240 metres
	Map Ref.:	Sheet No. : 8257   GPS	Rainfall:	No Data
	Northing/Long.:	7759225 AMG zone: 55	Runoff:	Moderately rapid
	Easting/Lat.:	469370  Datum: AGD66	Drainage:	Well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Undulating rises 9-30m 3-10%	Pattern Type:	Rises
	Morph. Type:	Upper-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	Very gently sloped
	Slope:	3 % 	Aspect:	130 degrees
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Eutrophic Red Chromosol Medium Non-gravelly Loamy 	Principal Profile Form:	Db1.22
	Clayey Shallow
	ASC Confidence:	Great Soil Group:	Solodic soil
	No analytical data are available but confidence is fair.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.51-1m, Sparse. *Species includes - Bothriochloa ewartiana, Bothriochloa pertusa, 
	Heteropogon contortus	Mid Strata - Tree, 3.01-6m, Sparse. *Species includes - Eucalyptus crebra, Eucalyptus erythrophloia
	Tall Strata - Tree, 12.01-20m, Sparse. *Species includes - Eucalyptus crebra, Eucalyptus erythrophloia
	Surface Coarse Fragments:	10-20%, fine gravelly, 2-6mm, angular, Granulite
	Profile Morphology
	A1	0 - 0.1 m	Dark brown (10YR3/3-Moist); ; Coarse sandy loam; Weak grade of structure, 5-10 mm, 
	Subangular blocky; Smooth-ped fabric; Dry; Very firm consistence; 0-2%, fine gravelly, 2-6mm, 
	angular, Quartz, coarse fragments; , Calcareous, , ; , Gypseous, , ; Field pH 7 (Raupach, 0.05); 
	Clear, Smooth change to - 
	A3	0.1 - 0.2 m	Brown (10YR4/3-Moist); ; Coarse sandy clay loam; Moderate grade of structure, 10-20 mm, 
	Subangular blocky; Smooth-ped fabric; Dry; Very firm consistence; 0-2%, fine gravelly, 2-6mm, 
	angular, Quartz, coarse fragments; , Calcareous, , ; , Gypseous, , ; Abrupt, Smooth change to - 
	B21	0.2 - 0.4 m	Dark yellowish brown (10YR4/4-Moist); ; Coarse sandy medium clay; Strong grade of structure,
	 10-20 mm, Angular blocky; Smooth-ped fabric; Dry; Strong consistence; 2-10%, fine gravelly, 
	2-6mm, angular, Quartz, coarse fragments; , Calcareous, , ; , Gypseous, , ; Field pH 7 
	(Raupach, 0.3); Clear, Smooth change to - 
	B/C	0.4 - 0.75 m	Dark yellowish brown (10YR4/4-Moist); Substrate influence, 10YR83, 10-20% , 0-5mm, 
	Prominent; Substrate influence, 10-20% ; Coarse sandy light clay; Moderate grade of structure, 
	10-20 mm, Subangular blocky; Smooth-ped fabric; Dry; Very firm consistence; 10-20%, medium 
	gravelly, 6-20mm, angular, Quartz, coarse fragments; , Calcareous, , ; , Gypseous, , ; Field pH 7
	 (Raupach, 0.6); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	364	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	364	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile