Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	368	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M. DeCorte	Locality:
	Date Desc.:	12/08/91	Elevation:	240 metres
	Map Ref.:	Sheet No. : 8257   GPS	Rainfall:	No Data
	Northing/Long.:	7756398 AMG zone: 55	Runoff:	Slow
	Easting/Lat.:	473113  Datum: AGD66	Drainage:	Well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Undisturbed soil core, Granodiorite 
	Land Form
	Rel/Slope Class: 	Undulating rises 9-30m 3-10%	Pattern Type:	Rises
	Morph. Type:	Mid-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	Very gently sloped
	Slope:	3 % 	Aspect:	240 degrees
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Eutrophic Red Chromosol Medium Non-gravelly Sandy 	Principal Profile Form:	Dr2.12
	Clayey Shallow
	ASC Confidence:	Great Soil Group:	Non-calcic brown
	No analytical data are available but confidence is fair.	 soil
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.51-1m, Sparse. *Species includes - Bothriochloa pertusa
	Mid Strata - Tree, 1.01-3m, Sparse. *Species includes - Eucalyptus crebra, Eucalyptus erythrophloia
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - Eucalyptus crebra, Eucalyptus erythrophloia, Eucalyptus 
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.08 m	Dark brown (7.5YR3/2-Moist); ; Loamy coarse sand; Moderate grade of structure, 2-5 mm, 
	Polyhedral; Smooth-ped fabric; Dry; Firm consistence; 0-2%, fine gravelly, 2-6mm, angular, 
	dispersed, Quartz, coarse fragments; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 
	0.05); Clear, Smooth change to - 
	A3	0.08 - 0.15 m	Dark brown (7.5YR3/3-Moist); ; Loamy coarse sand (Heavy); Moderate grade of structure, 5-10
	 mm, Polyhedral; Smooth-ped fabric; Dry; Firm consistence; 0-2%, fine gravelly, 2-6mm, angular,
	 dispersed, Quartz, coarse fragments; , Calcareous, , ; , Gypseous, , ; Abrupt, Smooth change 
	B21	0.15 - 0.45 m	Dark red (2.5YR3/6-Moist); ; Medium clay; Strong grade of structure, 20-50 mm, Angular blocky;
	 Smooth-ped fabric; Moderately moist; Strong consistence; Common cutans, 10-50% of ped 
	faces or walls coated, prominent; , Calcareous, , ; , Gypseous, , ; Field pH 7 (Raupach, 0.3); 
	Clear, Smooth change to - 
	BC	0.45 - 0.8 m	Red (2.5YR4/6-Moist); Substrate influence, 10YR83, 20-50% , 5-15mm, Prominent; Substrate 
	influence, 7.5YR58, 20-50% ; Sandy clay loam; Strong grade of structure, 20-50 mm, 
	Subangular blocky; Smooth-ped fabric; Moderately moist; Firm consistence; , Calcareous, , ; , 
	Gypseous, , ; Field pH 7.5 (Raupach, 0.6); Clear, Smooth change to - 
	C	0.8 - 1 m	; , Calcareous, , ; , Gypseous, , ; Field pH 7.5 (Raupach, 0.9); 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	368	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	368	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile