Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	376	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Site Information
	Desc. By:	M. DeCorte	Locality:
	Date Desc.:	13/08/91	Elevation:	260 metres
	Map Ref.:	Sheet No. : 8257   GPS	Rainfall:	No Data
	Northing/Long.:	7740596 AMG zone: 55	Runoff:	Rapid
	Easting/Lat.:	474004  Datum: AGD66	Drainage:	Moderately well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Existing vertical exposure, Siltstone 
	Land Form
	Rel/Slope Class: 	Gently undulating rises 9-30m  	Pattern Type:	Rises
	1-3%
	Morph. Type:	Lower-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	Gently inclined
	Slope:	3 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Eutrophic Mesonatric Brown Sodosol Thick Very gravelly Silty	Principal Profile Form:	Dy3.43
	 Clayey Moderately deep
	ASC Confidence:	Great Soil Group:	Solodic soil
	Analytical data are incomplete but reasonable confidence.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, <0.25m, Very sparse. *Species includes - None recorded
	Mid Strata - Tree, 1.01-3m, Sparse. *Species includes - Eremophila mitchellii
	Tall Strata - Tree, 6.01-12m, Mid-dense. *Species includes - Eucalyptus brownii
	Surface Coarse Fragments:	50-90%, medium gravelly, 6-20mm, angular, Siltstone
	Profile Morphology
	A1	0 - 0.15 m	Dark yellowish brown (10YR4/4-Moist); ; Silty loam; Massive grade of structure; Earthy fabric; 
	Dry; Strong consistence; , Calcareous, , ; , Gypseous, , ; Field pH 6 (Raupach, 0.05); Clear, 
	Smooth change to - 
	A2	0.15 - 0.3 m	Yellowish brown (10YR5/4-Moist); ; Silty loam; Massive grade of structure; Earthy fabric; Dry; 
	Strong consistence; 0-2%, fine gravelly, 2-6mm, angular, dispersed, Siltstone, coarse 
	fragments; , Calcareous, , ; , Gypseous, , ; Field pH 6.5 (Raupach, 0.3); Abrupt, Smooth change 
	B1	0.3 - 0.42 m	Yellowish brown (10YR5/4-Moist); Mottles, 0-2% , 0-5mm, Distinct; Mottles, 0-2% ; Medium clay;
	 Strong grade of structure, 20-50 mm, Angular blocky; Smooth-ped fabric; Dry; Very strong 
	consistence; 10-20%, fine gravelly, 2-6mm, angular, dispersed, Siltstone, coarse fragments; , 
	Calcareous, , ; , Gypseous, , ; Gradual, Smooth change to - 
	B21	0.42 - 0.75 m	Yellowish brown (10YR5/6-Moist); ; Medium clay; Moderate grade of structure, 50-100 mm, 
	Angular blocky; Smooth-ped fabric; Dry; Very strong consistence; 10-20%, fine gravelly, 2-
	6mm, angular, dispersed, Siltstone, coarse fragments; , Calcareous, , ; , Gypseous, , ; Field pH 
	9.5 (Raupach, 0.6); Clear, Smooth change to - 
	C	0.75 - 0.9 m	; , Calcareous, , ; , Gypseous, , ; 
	Morphological Notes
	Observation Notes
	Site Notes

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	376	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0.42 - 0.75	8.7A	0.8J	4.4	0.2	1.7	6.5I	26.15
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0.42 - 0.75
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0.42 - 0.75

	Project Name:	Preliminary Assessment and Survey of Land Degradation in the Dalrypmle Shire, QLD
	Project Code:	DLR	Site ID:	376	Observation ID:	1
	Agency Name:	QLD Department of Primary Industries
	Laboratory Analyses Completed for this profile
	15F1_CA	Exchangeable bases by 0.01M silver-thiourea (AgTU)+, no pretreatment for soluble salts
	15F1_K	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_MG	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F1_NA	Exchangeable bases by 0.01m (AgTU)+, no pretreatment for soluble salts
	15F3	CEC by 0.01M silver-thiourea (AgTU)+
	15N1	Exchangeable sodium percentage (ESP)
	4A1	pH of 1:5 soil/water suspension